Permit Number: EPR/SP3537VQ





Operator: Biogen (UK) Ltd
Facility: Biogen Bryn Pica







Form Number: Air1 16/01/14
Reporting of emissions to air for the period from 01/01/2015 to 31/12/2015 
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	A1 CHP Exhaust
	Oxides of Nitrogen
	500 mg/m3
	Hourly mean
	n/a
	BS EN 14792
	n/a
	n/a

	A1 CHP Exhaust
	Carbon Monoxide
	1400 mg/m3
	Hourly mean
	n/a
	BS EN 15058
	n/a
	n/a

	A1 CHP Exhaust
	Sulphur Dioxide
	350 mg/m3
	Hourly mean
	n/a
	BS EN 14791
	n/a
	n/a

	A1 CHP Exhaust
	VOCs
	1000 mg/m3
	Hourly mean
	n/a
	 BS EN 12619:1999 or 13526:2002 depending on concentration
	n/a
	n/a

	A2 Flare Stack
	Oxides of Nitrogen
	150 mg/m3
	Hourly mean
	n/a
	BS EN 14792
	n/a
	n/a

	A2 Flare Stack
	Carbon Monoxide
	50 mg/m3
	Hourly mean
	n/a
	BS EN 15058
	n/a
	n/a

	A2 Flare Stack
	VOCs
	10 mg/m3
	Hourly mean
	n/a
	BS EN 12619:1999 or BS EN 13526:2002
	n/a
	n/a


The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.

For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.
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	Operator’s comments :

A request to reschedule the MCERTs emission testing for Bryn Pica to April 2016 was communicated to Gwyn Jones of the NRW on the 27th October 2015. This was due to the fact that the CHP had not yet been operational for a full calendar years as operation commenced in May 2015. A written approval to postpone the testing was received from Gwyn Jones on the 27th of October 2015. Further communication was received from Gwyn Jones on the 7th of March 2016 requesting a nil return for the 2015 Air Report. As such, the above has been submitted. A full report detailing the annual emissions from the CHP and Flare stack will therefore be submitted following the test and the submission shall be made by the 28th of Jan 2017 as per Gwyn Jones email dated 7th March 2016. 


Signed: Esther Hombarume (Environment Manager)                                                                                                                                  Date: 14/03/2016   



(Authorised to sign as representative of Operator)

