Maxibrite Limited 

Monthly Site Housekeeping Report 68 – December 2015 Period
Volume Reduction of Raw Material Coal Fines Stored On Site Via Processing
Following on from Report 67, the total of finer/wetter particle size coal fines processed via the rotary dryer during this period was circa 1027tonnes, pending completion of monthly production figures. 
Site Housekeeping Actions
The general site clean-up has continued during the month, with internal and external plant areas cleaned to concrete, prior to further inspection/ maintenance and safety work. Additional redundant pieces of plant, equipment and cabling have continued to be removed. The roadway to lagoon 3 has been kept clear/accessible. Lagoons 1 and 2 have been cleaned out of solids to optimise gravity settlement. 
The effluent filter press performance has continued to be monitored whilst using the new higher pressure lagoon 3 pump.

The site roadways have been periodically wetted and cleaned to concrete via recycled water hoses, along with plant areas.  The dust suppression sprays have continued to be in operation during periods of dry weather to prevent any fugitive dust releases, along with machine buckets of water/rain gun. 
Small sections of sheeting on the main plant building have been renewed. In addition, sections of the rotary dryer exhaust stack have been renewed in stainless steel. 
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