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Permit with introductory note
The Environmental Permitting (England & Wales) Regulations 2016

Mr Martin Evans

Domgay Hall Broiler Unit 
Domgay Hall
Four Crosses
Powys
SY22 6SN



Permit number
EPR/AB3696CC




Permit Number   EPR/AB1234CD	  	
[bookmark: _Toc77056945]
Domgay Hall Broiler Unit
Permit number EPR/AB3696CC

Introductory note

This introductory note does not form a part of the permit
The main features of the permit are as follows.  

Domgay Hall Broiler Unit proposes to operate as a broiler meat production unit with capacity for 100,000 chickens per crop cycle and an annual meat production capacity of 1,578 tonnes and an annual manure production capacity of around 1,800 tonnes.

There will be two fan ventilated poultry houses, this will give a bird stocking density of approximately 100,000 under the current legislative/welfare stocking density. The proposed poultry houses will each be ventilated by 6 high velocity roof fans (12 high velocity roof fans in total) and 5 gable end fans (10 gable end fans in total). The working area where vehicles operate is laid to concrete and hard standing. Feed is delivered in covered lorries and stored on site in vermin proof steel galvanised bins. Manure is removed from houses at the end of the production cycle. Immediately following depopulation, litter is removed off site, for use on operator controlled land or sold to a local Anaerobic Digester. The houses are then washed and disinfected prior to the cycle beginning again. An underground storage tank will have been installed to catch all wash waters. Dead birds are removed from the houses and stored in sealed containers awaiting collection from a licensed renderer. Diesel fuel storage is in a bunded tank, Chemicals are stored in a frost free secure bunded store (off site).

The footprint of the proposed intensive development will be totalling approximately 0.51 hectares (ha) within a site of 1.187ha. The buildings will 5.0m high and the associated feed bins 8m high. Hours of operation will be 24 hours a day 7 days a week due to the fact that it is a livestock enterprise requiring continual husbandry. Short seven day periods between crop cycles will occur when there will be no birds on the site.

The status log of the permit sets out the permitting history, including any changes to the permit reference number.

	Status log of the permit

	Description
	Date
	Comments

	Application received EPR/AB3696CC/A001
	Duly made 24/05/17
	Application for 100,000 broiler places installations permit

	Additional information received
	26/10/17
	Site drainage plan and point source emissions to air.

	Permit determined EPR/AB3696CC
	18/12/17
	EPR/AB3696CC Permit issued to Mr Martin Evans



End of introductory note


Intensive Farming Sector Specific Conditions Set 1  (version March 2017)



Permit Number   EPR/AB3696CC	 Page 22	18/12/17


	
Permit


The Environmental Permitting (England and Wales) Regulations 2016

Permit number 
EPR/AB3696CC
The Natural Resources Body for Wales (“Natural Resources Wales”) authorises, under regulation 13 of the Environmental Permitting (England and Wales) Regulations 2016 
[bookmark: OperatorName2]
Mr Martin Evans (“the operator”),

[bookmark: InstallationAddress21]of

Domgay Hall
Four Crosses
Powys
SY22 6SN

to operate an installation at

Domgay Hall Broiler Unit
Domgay Hall
Four Crosses
Powys
SY22 6SN

to the extent authorised by and subject to the conditions of this permit as set out in Appendix 1 and in Appendix 2.


	Signed
	Date

	[image: ]
	18/12/2017


Anna Lewis, Principal Permitting Officer
Authorised on behalf of Natural Resources Wales

APPENDIX 1
Sector Specific Conditions 
Introductory note
This introductory note does not form a part of the Condition set
The conditions set out below are incorporated into this permit.
End of introductory note.

1 Management
1.1 General management
1.1.1 The operator shall manage and operate the activities:
(a) in accordance with a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances, closure and those drawn to the attention of the operator as a result of complaints; and
(b) using sufficient competent persons and resources.
1.1.2 Records demonstrating compliance with condition 1.1.1 shall be maintained. 
1.1.3 Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of it kept at or near the place where those duties are carried out.

1.2	Energy efficiency

1.2.1	The operator shall:
(a)	take appropriate measures to ensure that energy is used efficiently in the activities;
 (b)	review and record at least every four years whether there are suitable opportunities to improve the energy efficiency of the activities; and  
(c)	take any further appropriate measures identified by a review. 

1.3    Efficient use of raw materials

1.3.1	The operator shall: 

(a)	take appropriate measures to ensure that raw materials and water are used efficiently in the activities; 
(b)	maintain records of raw materials and water used in the activities;
(c)	review and record at least every four years whether there are suitable alternative materials that could reduce environmental impact or opportunities to improve the efficiency of raw material and water use; and
(d)	take any further appropriate measures identified by a review.
1.4	Avoidance, recovery and disposal of wastes produced by the activities
1.4.1 The operator shall take appropriate measures to ensure that:
(a)	the waste hierarchy referred to in Article 4 of the Waste Framework Directive is applied to the generation of waste by the activities; and
(b)	any waste generated by the activities is treated in accordance with the waste hierarchy referred to in Article 4 of the Waste Framework Directive; and
(c)	where disposal is necessary, this is undertaken in a manner which minimises its impact on the environment.
1.4.2 The operator shall review and record at least every four years whether changes to those measures should be made and take any further appropriate measures identified by a review.

2	Operations
2.1	Permitted activities
2.1.1	The operator is only authorised to carry out the activities specified in schedule 1 table S1.1 (the “activities”). 

2.2	The site
See Appendix 2.
2.3	Operating techniques
2.3.1	(a) 	The activities shall, subject to the conditions of this permit, be operated using the techniques and in the manner described in the documentation specified in schedule 1, table S1.2, unless otherwise agreed in writing by Natural Resources Wales.
(b)	If notified by Natural Resources Wales that the activities are giving rise to pollution, the operator shall submit to Natural Resources Wales for approval within the period specified, a revision of any plan specified in schedule 1, table S1.2 or otherwise required under this permit which identifies and minimises the risks of pollution relevant to that plan , and shall implement the approved revised plan in place of the original from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
2.3.2	The operator shall maintain and implement a system to record the number of animal places and animal movements.
2.3.3	The operator shall maintain and implement a system to record the quantities of solid manure or slurry exported from the installation, as defined on the site plan in schedule 7.  The record shall include as a minimum:
· the date of export from the site
· the quantity exported 
· details of the receiving site

2.3.4	The operator shall ensure that where waste produced by the activities is sent to a relevant waste operation, that operation is provided with the following information, prior to the receipt of the waste:
	(a)	the nature of the process producing the waste;
	(b)	the composition of the waste;
	(c)	the handling requirements of the waste;
	(d)	the hazardous property associated with the waste, if applicable; and
	(e)	the waste code of the waste.
2.3.5	The operator shall ensure that where waste produced by the activities is sent to a landfill site, it meets the waste acceptance criteria for that landfill.
2.3.6      The operator shall ensure that a diet formulation and a nutritional strategy is used that minimises as far as is practicable the amount of Phosphorus and Nitrogen excreted.

3	Emissions and monitoring
3.1	Emissions to water, air or land
3.1.1	There shall be no point source emissions to water, air or land except from the sources and emission points listed in tables S3.2, S3.3 and S3.4.
3.2 Emissions of substances not controlled by emission limits
3.2.1 Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.
3.2.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution, submit to Natural Resources Wales for approval within the period specified, an emissions management plan which identifies and minimises the risks of pollution from emissions of substances not controlled by emission limits;
(b)	implement the approved emissions management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.2.3	All liquids in containers, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the operator has used other appropriate measures to prevent or where that is not practicable, to minimise, leakage and spillage from the primary container.
3.2.4 Periodic monitoring shall be carried out at least once every 5 years for groundwater and 10 years for soil, unless such monitoring is based on a systematic appraisal of the risk of contamination.

3.3	Odour
3.3.1	Emissions from the activities shall be free from odour at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved odour management plan, to prevent or where that is not practicable to minimise the odour. 
3.3.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to odour, submit to Natural Resources Wales for approval within the period specified, an odour management plan which identifies and minimises the risks of pollution from odour;
(b)	implement the approved odour management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.

3.4	Noise and vibration
3.4.1	Emissions from the activities shall be free from noise and vibration at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved noise and vibration management plan to prevent or where that is not practicable to minimise the noise and vibration.
3.4.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to noise and vibration, submit to Natural Resources Wales for approval within the period specified, a noise and vibration management plan which identifies and minimises the risks of pollution from noise and vibration;
(b)	implement the approved noise and vibration management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.

3.5	Monitoring 
3.5.1	The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring specified in the following tables:
(a) emissions specified in tables S3.1, S3.2, S3.3 and S3.4.
3.5.2	The operator shall maintain records of all monitoring required by this permit including records of the taking and analysis of samples, instrument measurements (periodic and continual), calibrations, examinations, tests and surveys and any assessment or evaluation made on the basis of such data.
3.6	Pests
3.6.1 	The activities shall not give rise to the presence of pests which are likely to cause pollution, hazard or annoyance outside the boundary of the site. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved pests management plan, have been taken to prevent or where that is not practicable, to minimise the presence of pests on the site.  
3.6.2 	The operator shall:	
(a)          if notified by Natural Resources Wales, submit to Natural Resources Wales for approval within the period specified, a pests management plan which identifies and minimises risks of pollution, hazard and annoyance from pests;
(b)          implement the pests management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
[bookmark: _Toc77056949]4	Information
4.1	Records
4.1.1 All records required to be made by this permit shall:
(a) be legible;
(b) be made as soon as reasonably practicable;
(c) if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
(d) be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made, or in the case of the following records until permit surrender:
(i) off-site environmental effects; and
(ii) matters which affect the condition of the land and groundwater.
4.1.2 The operator shall keep on site all records, plans and the management system required to be maintained by this permit, unless otherwise agreed in writing by Natural Resources Wales. 

4.2	Reporting
4.2.1	The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
4.2.2	A report or reports on the performance of the activities over the previous year shall be submitted to Natural Resources Wales by 31 January (or other date agreed in writing by Natural Resources Wales) each year.  The report(s) shall include as a minimum:
(a)	a review of the results of the monitoring and assessment carried out in accordance with the permit including an interpretive review of that data; 
(b)	the annual production /treatment data set out in schedule 4 table S4.2; and
(c)	the performance parameters set out in schedule 4 table S4.3 using the forms specified in table S4.4 of that schedule.
4.2.3	The operator shall, unless notice under this condition has been served within the preceding four years, submit to Natural Resources Wales, within six months of receipt of a written notice, a report assessing whether there are other appropriate measures that could be taken to prevent, or where that is not practicable, to minimise pollution.

4.3	Notifications
4.3.1	(a) 	In the event that the operation of the activities gives rise to an incident or accident which significantly affects or may significantly affect the environment, the operator must immediately:
		(i) 	inform Natural Resources Wales; 
		(ii)	take the measures necessary to limit the environmental consequences of such an incident or accident; and
(iii) take the measures necessary to prevent further possible incidents or accidents.


	(b)	In the event of a breach of any permit condition the operator must immediately:
		(i) 	inform Natural Resources Wales; and,
		(ii)	take the measures necessary to ensure that compliance is restored within the shortest possible time.
	(c) 	In the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment, the operator must immediately suspend the operation of the activities or the relevant part of it until compliance with the permit conditions has been restored.
4.3.2       Any information provided under condition 4.3.1, shall be confirmed by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
4.3.3	Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.
4.3.4	Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules: 
Where the operator is a registered company:
(a) any change in the operator’s trading name, registered name or registered office address; and
(b)	any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) 	any change in the operator’s name or address; and
(b) any steps taken with a view to the dissolution of the operator.	
In any other case: 
(a) the death of any of the named operators (where the operator consists of more than one named individual);
(b)        any change in the operator’s name(s) or address(es); and
(c) any steps taken with a view to the operator, or any one of them, going into bankruptcy, entering into a composition or arrangement with creditors, or, in the case of them being in a partnership, dissolving the partnership.
4.3.5	Where the operator proposes to make a change in the nature or functioning, or an extension of the activities, which may have consequences for the environment and the change is not otherwise the subject of an application for approval under the Regulations or this permit:
(a) Natural Resources Wales shall be notified at least 14 days before making the change; and
(b) the notification shall contain a description of the proposed change in operation.
4.3.6	Natural Resources Wales shall be given at least 14 days notice before implementation of any part of the site closure plan.
 4.4	Interpretation
4.4.1	In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
4.4.2	In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “without delay”, in which case it may be provided by telephone.



Schedule 1
Operations

See Appendix 2


Schedule 2
Waste types, raw materials and fuels

See Appendix 2


Schedule 3
Emissions and Monitoring

	Table S3.1  BAT associated emission levels and monitoring requirements Note 1

	

	Emission point ref. & location
	Parameter  
	Source
	Limit (incl. unit) 
	Reference period
	Monitoring frequency
	Monitoring standard or method

	Weaners
	Nitrogen
(N)
	Excreted 
	4.0 kg N
/animal place
	Per  year
	Annually 
	Calculation by using a mass balance of nitrogen and phosphorus based on the feed intake, dietary content of crude protein, total phosphorus and animal performance or
Estimation by using manure analysis for total nitrogen and total phosphorus content 

	
	Phosphorus (as P2O5)
	Excreted
	2.2 kg  P2O5 /animal place
	Per year
	Annually
	As above

	
	Ammonia
(as NH3)
	Animal house
	0.53 kgNH3
/animal place
	Per year
	Annually
	Estimation using emission factors

	Fattening Pigs
	Nitrogen
(N)
	Excreted
	13.0 kg N
/animal place
	Per year-
	Annually
	Calculation by using a mass balance of nitrogen and phosphorus based on the feed intake, dietary content of crude protein, total phosphorus and animal performance or
Estimation by using manure analysis for total nitrogen and total phosphorus content

	
	Phosphorus (as P2O5)
	Excreted
	5.4 kg P2O5 /animal place
	Per year
	Annually
	As above

	
	Ammonia
(as NH3)
	Animal house
	2.6 kg NH3
/animal place
	Per year
	Annually
	Estimation using emission factors

	Sows (including suckling piglets)
	Nitrogen
(N)
	Excreted
	30.0 kg N
/animal place
	Per year
	Annually
	Calculation by using a mass balance of nitrogen and phosphorus based on the feed intake, dietary content of crude protein, total phosphorus and animal performance or
Estimation by using manure analysis for total nitrogen and total phosphorus content

	
	Phosphorus (as P2O5)
	Excreted
	15 kg P2O5
/animal place
	Per year
	Annually
	As above

	Mating and gestating sows
	Ammonia
(as NH3)
	Animal house
	2.7 kg NH3
/animal place
	Per year
	Annually
	Estimated using excretion factors

	Farrowing sows (including suckling piglets) with crates.
	Ammonia
(as NH3)
	Animal house
	5.6 kg NH3
/animal place
	Per year
	Annually
	Estimated using excretion factors

	Laying hens
	Nitrogen
(N)
	Excreted
	0.8 kg N
/animal place
	Per year
	Annually
	Calculation by using a mass balance of nitrogen and phosphorus based on the feed intake, dietary content of crude protein, total phosphorus and animal performance or
Estimation by using manure analysis for total nitrogen and total phosphorus content

	
	Phosphorus (as P2O5)
	Excreted
	0.45 kg/P2O5
/animal place
	Per year
	Annually
	As above

	Laying hens in Caged housing
	Ammonia
(as NH3)
	Animal house
	0.08 kg NH3
/animal place
	Per year
	Annually
	Estimation by using emission factors

	Laying hens in Non caged housing
	Ammonia
(as NH3)
	Animal house
	0.13 kg NH3
/animal place
	Per year
	Annually
	Estimation by using emission factors

	Broilers
	Nitrogen
(N)
	Excreted
	0.6 kg N
/animal place 
	Per year
	Annually
	Calculation by using a mass balance of nitrogen and phosphorus based on the feed intake, dietary content of crude protein, total phosphorus and animal performance or
Estimation by using manure analysis for total nitrogen and total phosphorus content

	
	Phosphorus (as P2O5)
	Excreted
	0.25 kg P2O5
/animal place
	Per year
	Annually
	As above

	
	Ammonia
(as NH3)
	Animal house
	0.08 kg NH3
/animal place
	Per year
	Annually
	Estimation by using emission factors

	Ducks
	Nitrogen
(N)
	Excreted
	0.8 kg N
/animal place
	Per year
	Annually
	Calculation by using a mass balance of nitrogen and phosphorus based on the feed intake, dietary content of crude protein, total phosphorus and animal performance or
Estimation by using manure analysis for total nitrogen and total phosphorus content

	Turkeys
	Nitrogen
(N)
	Excreted
	2.3 kg N
/animal place 
	Per year
	Annually
	Calculation by using a mass balance of nitrogen and phosphorus based on the feed intake, dietary content of crude protein, total phosphorus and animal performance or
Estimation by using manure analysis for total nitrogen and total phosphorus content

	
	Phosphorus (as P2O5)
	Excreted
	1.0 kg P2O5
/animal place
	Per Year
	Annually
	As above


Note 1.  There are no BAT emission factors specified for pullets.


Table S3.2 – Point source emissions to air emissions limits and monitoring requirements - see Appendix 2.
Table S3.3 – Point source emissions to water (other than sewer) – emission limits and monitoring – see Appendix 2.       
Table S3.4 – Point source emissions to land – emission limits and monitoring – see Appendix 2           


Schedule 4
Reporting

See Appendix 2
Schedule 5 - Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A 
	Permit Number
	

	Name of operator
	

	Location of Facility
	

	Time and date of the detection 
	



	(a) Notification requirements for any activity that gives rise to an incident or accident which significantly affects or may significantly affect the environment

	To be notified within 24 hours

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



	(b) Notification requirements for the breach of a permit condition

	To be notified within 24 hours

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	



	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	



	(c) In the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment:

	To be notified within 24 hours

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	



Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator


Schedule 6 - Interpretation 
“accident” means an accident that may result in pollution.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“authorised officer” means any person authorised by Natural Resources Wales under section 108(1) of The Environment Act 1995 to exercise, in accordance with the terms of any such authorisation, any power specified in section 108(4) of that Act.
“BAT” means “best available techniques” as detailed in the Commission Implementing Decision (EU) 2017/302 of 15 February 2017.
 “building” means a construction that has the objective of providing sheltering cover and minimising emissions of noise, particulate matter, odour and litter.
“emissions to land” includes emissions to groundwater.
“emission factors” are figures which have been agreed in writing with Natural Resources Wales and can be used in specific calculations.
“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the activities, either from the emission points specified in schedule 3 or from other localised or diffuse sources, which are not controlled by an emission limit..
“excretion factors” are figures which have been agreed in writing with Natural Resources Wales and can be used in specific calculations. 
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.675 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.
“Industrial Emissions Directive” means DIRECTIVE 2010/75/EU OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 24 November 2010 on industrial emissions
“Manure and slurry” have the following meaning:
· Manures may be either slurries or solid manures.
· Slurries consist of excreta produced by livestock whilst in a yard or building mixed with rainwater and wash water and, in some cases, waste bedding and feed. Slurries can be pumped or discharged by gravity. 
· Slurry includes muck effluent, seepage from manure and wash water.
· Solid manures include farmyard manure (FYM) and comprise material from straw-based housing systems, excreta with lots of straw/sawdust/woodchips in it, or solids from mechanical separators. 
· Most poultry systems produce solid manure (litter).
· Solid manure can generally be stacked.
“Manure management plan” means the requirements described in Section 2.3 of SGN 6.09 How to Comply – Intensive Farming.  
“Pests” means Birds, Vermin and Insects.
 “SGN How to comply – Intensive Farming” The EPR Sector Guidance Note 6.09 for intensive pig and poultry farmers, version 2 published January 2010. 
“year” means calendar year ending 31 December.




Schedule 7 – Site plan – see Appendix 2



































APPENDIX 2
Site Specific Conditions 
Introductory note
This introductory note does not form a part of the Condition set
The conditions set out below are incorporated into this permit.
End of introductory note.

2	Operations
		2.2	The site 
2.2.1	The activities shall not extend beyond the site, being the land shown edged in green on the site plan at schedule 7 to this permit.


Schedule 1 - Operations 
 
 
	Table S1.1 activities
	
	

	Activity listed in Schedule 1 of the EP Regulations 
	Description of specified activity
	Limits of specified activity 

	Section 6.9 A(1)(a) Rearing of poultry or pigs intensively in an installation with more than 40,000 places for poultry. 
	The rearing of poultry in a broiler facility. 
	To house a maximum capacity of 100,000 broiler birds. From receipt of birds, raw materials and fuels onto the site, to removal of birds and associated wastes from site.

	Directly Associated Activity

	Biomass Boiler 
	Operation of Biomass Boiler with a thermal rated input of 990kW for site heating.
	From receipt of raw materials and
fuels, to release of combustion
products to air and associated
wastes removed from site.

	Dirty water tank
	Storage of dirty water from washing of poultry houses.
	Temporary storage of wash down water.

	Fuel tank
	Storage of fuel
	Fuel to be stored in bunded fuel tank.

	Feed silos
	Feed storage
	Feed is stored in 6 vermin proof steel galvanised bins.










	Table S1.2 Operating techniques

	Description
	Parts
	Date Received

	Application PAN-001438
	Part B2 and B3 of the application and all referenced supporting documents.

	31/03/17

	Application PAN-001438
	Odour Management Plan, Noise and Vibration Management Plan, Environmental Management System, Manure Management Plan.

	31/03/17

	Response to Schedule 5 Notice dated 02/08/17
	Response to Schedule 5 detailing site Drainage Plan and Point Source Emissions to Air.
	28/09/17

	Application PAN-001438
	Revised Site Plan
	11/11/17





Schedule 2 - Waste types, raw materials and fuels

	Table S2.1 Raw materials and fuels
	

	Raw materials and fuel description 
	Specification

	Fuel for biomass boiler units
	Virgin timber woodchip or biomass pellets comprising only virgin timber, straw, miscanthus or a combination of these. 
 
Not to include any waste material or animal carcasses. 




  	Schedule 3 – Emissions and Monitoring

	Table S3.2  Point source emissions to air – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter
	Limit (incl. unit) 
	Reference period
	Monitoring frequency
	Monitoring standard or method

	High velocity roof fan outlets as shown on the site plan in schedule 7
	Poultry houses 1 and 2
	None set
	None set
	None set
	None set
	None set

	Gable end fan outlets as shown on the site plan in schedule 7
	Poultry houses 1 and 2
	None set
	None set
	None set
	None set
	None set

	Exhaust chimney from Biomass Boiler as shown on the site plan in schedule 7
	Biomass Boiler
	None set
	None set
	None set
	None set
	None set





	Table S3.3 Point Source emissions to water (other than sewer) – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter
	Limit (incl. unit)
	Reference Period
	Monitoring frequency
	Monitoring standard or method

	Discharge to unnamed tributary of the River Vyrnwy as shown on the site drainage plan
	Clean, uncontaminated rainwater draining from the roofs of poultry houses and yard area.
	None set
	None set
	None set
	None set
	None set





	Table S3.4 Point Source emissions to land – emission limits and monitoring requirements

	Emission point ref. & location
	Source  
	Parameter
	Limit (incl. unit)
	Reference Period
	Monitoring frequency
	Monitoring standard or method

	Outlet from clean water drains discharging to balancing pond as shown on the site drainage plan
	Clean, uncontaminated rainwater draining from the roofs of poultry houses and yard area
	None set
	None set
	None set
	None set
	None set


Schedule 4 - Reporting
Parameters, for which reports shall be made, in accordance with conditions of this permit, are listed below.

	Table S4.1 Reporting of monitoring data

	Parameter
	Emission or monitoring point/reference
	Reporting period
	Period begins

	As detailed in table S3.1 and as applicable to your operation
	As detailed in table S3.1 and as applicable to your operation
	Annually
	1 January




	Table S4.2: Annual production/treatment

	Parameter
	Units 

	Live birds removed from site
	Birds




	Table S4.3 Performance parameters

	Parameter
	Frequency of assessment
	Units

	Ammonia 
	Annually
	kg NH3/animal place/year 

	Total Nitrogen excreted
	Annually
	kg N excreted/animal place/year

	Total Phosphorus excreted
	Annually
	kg P2O5 excreted/animal place/year




	Table S4.4 Reporting forms

	Media/parameter
	Reporting format
	Date of form

	kg N excreted/animal place/year 
and 
kg P2O5 excreted/animal place/year
	Form N&P Excretion 1 or other form as agreed in writing by Natural Resources Wales
	18/12/17

	kg NH3/animal place/year
	Form Air 1 or other form as agreed in writing by Natural Resources Wales 
	[bookmark: _GoBack]18/12/17
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