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DOW CORNING LTD
SCHEDULE  5 PART A  INCIDENT NOTIFICATION

This information MUST be FAXED to the Natural Resources Wales at the below FAX no. within 24 hr. of an incident occurring. 









Revision Date:   06 June 2006
	To:
	Process Industry Inspector

	FAO: Mr Tony Leakey
	Natural Resources Wales
Rivers House

St Mellons Business Park

Fortran Road

St Mellons

Cardiff

CF3 0EY

	FAX No:
	029 20362095

	From:

	Helen Gough

	Name Of Operator
	Dow Corning Limited

	Location of Process:

	Cardiff Road, Barry, Vale of  Glamorgan

	FAX No:
	01446-749634

	Telephone No:
	01446-723842

	Date Information Provided:
	8th January 2016


Part A

	Permit Number
	EPR/BR9685IX

	Name of Operator
	Dow Corning Ltd

	Location of Facility
	Barry, South Glamorgan, Wales

	Time and Date of Detection
	     10:00              7th January 2016


	a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	Date and time of event
	

	Reference or description of the location of the event
	

	Description of where any release into the environment took place
	

	Substance(s) potentially released
	

	Best estimate of quantities or rate of release
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident
	


	b) Notification requirements for the breach of a limit

	Emission point reference source
	Authorized vent A41

	Parameter(s)
	HCl and Chlorine

	Limit
	HCl – 10mg/m3 annual average / 15mg/m3 for individual monthly results
Cl  0 10mg/m3

	Measured value and uncertainty
	HCl - >20ppm draeger sample (~32+mg/m3)

Cl 7ppm dragger sample (~22mg/m3)

	Date and time of monitoring
	Samples taken early morning of 6th January

	Measures taken, or intended to be taken, to stop the emission
	Preliminary findings were undertaken;

W931 plant was in start-up with elevated vent levels being sent to the incinerator. In addition the fridge on this process tripped for a period of time.
Subsequent draeger testing was within permit levels. 

Draeger testing is notoriously unreliable but due to abnormal operating conditions of the incinerator with high flows it is possible that the environmental limit has been exceeded. Discussed with Tony Leakey 8th Jan 2016 and agreed a potential breach would be recorded.

Follow up investigation to be completed by Dow Corning to be reviewed at next quarterly compliance assessment by NRW, planned for early March.


	c) Notification requirements for the detection of any significant adverse environmental effect, to be notified within 24 hours.

	Description of where the effect on the environment was detected
	

	Substance(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	


Part B- to be submitted as soon as practicable
	Any more information on the matters for notification under Part A
	

	Measure taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measure taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment, which has been or may be caused by the emission.
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	


	Name
	Helen Gough

	Post
	Environmental Team Leader

	Signature
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	Date
	8th January 2016


