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	Permit Number:

	BR9715B

	Name of Operator:

	Solutia UK Ltd

	Location of Installation:

	Corporation Road, Newport, Gwent, NP194XF

	Location of the emission:

	Therminol 3 – CO2 vent

	Time and date of the emission:
	14/01/2018



	Substance(s) emitted
	Media
eg air /water
	Best estimate of the quantity or the rate of emission
	Time during which the emission took place

	Liquid Benzene & Biphenyl
	Discharge to ground (concrete), some would be as vapour
	Estimated ~36 L
	The liquid would have dripped from the pipework section for a short period of time (1 hr estimated)


 
	Measures taken, or intended to be taken, to stop the emission:
	Thought to be as a result of an unseated valve(s) allowing liquid to pass into the CO2 pipework. This pipework features a weep hole which has allowed the liquid to drip out onto the concrete beneath. The limited quantity was not sufficient to flow to drainage. Arrangement made to replace the valve & investigate prior to process restart. Additional info to follow in the Part B
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