Permit Number: 
BR8212IK





Operator: 

Knauf Insulation Ltd

Installation:

Knauf Insulation Ltd, Cwmbran


Form Number:
Sewer1  
Reporting of emissions to sewer for the period from 

01/07/2014
to
31/12/2014   
	Emission

Point
	Substance /

Parameter
	Emission

Limit Value
	Reference Period
	Result [1]
	Test

Method [2]
	Sample

Date and Times [3]
	Uncertainty

[4]

	S1
	COD
	6500 mg/l
	Spot sample
	1230 mg/l
	AES 1029
	14/11/2014

11:30
	​-

	S1
	Monohydric Phenols (as phenol)
	20 mg/l
	Spot sample
	0.09 mg/l
	AES 1021
	14/11/2014

11:30
	-

	S1
	Total suspended solids
	900 mg/l
	Spot sample
	111 mg/l
	AES 1041
	14/11/2014

11:30
	-

	S1


	Total sulphates


	900 mg/l


	Spot sample
	145 mg/l
	AES 1020
	14/11/2014

11:30
	-

	
	
	
	
	
	
	
	

	S1
	Total hydrocarbon oil
	650 mg/l
	Spot sample
	0.67 mg/l
	GC - FID
	14/11/2014

11:30
	-

	
	
	
	
	
	
	
	

	S1
	PH max

	12
	Spot sample
	7.21
	AES 1035
	14/11/2014

11:30
	-

	S1
	PH min
	6
	Spot sample
	7.21
	AES 1035
	14/11/2014

11:30
	-


[1]
The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.

[2]
Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with the Agency is used, then the appropriate identifier is given. In other cases the principal technique is stated, e.g. gas chromatography.

[3]
For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   

[4]
The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.

Signed …… …………………[image: image1.emf]…………………………………….  

Date……05/01/2015……..   



(Authorised to sign as representative of Operator)

