Schedule 5 - Notification 

This page outlines the information that the Operator must provide. 

Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.

If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.

Part A 
	Permit Number
	EPR/PR3733PC V007

	Name of Operator
	Biffa Waste Services Limited

	Location of Facility
	Trecatti Landfill Site

Fochriw Road

Merthyr Tydfil

Mid Glamorgan

CF48 4AB

	
	

	Time and date of the detection 
	27/01/2015


	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and Time of the event
	N/A

	Reference or description of the location of the event 
	N/A

	Description of where any release into the environment took place
	N/A

	Substances(s) potentially released
	N/A

	Best estimate of the quantity or rate of release of substances
	N/A

	Measures taken, or intended to be taken, to stop any emission
	N/A

	Description of the failure or accident.
	N/A


	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	81703040 Leachate Well 4

	Parameter(s)
	Leachate level

	Limit
	33m

	Measured value and uncertainty
	34.3m, 43.47m

	Date and time of monitoring
	3/11/2014, 9/12/2014

	Measures taken, or intended to be taken, to stop the emission
	 No Emission has taken place as a result of this breach



	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	Leachate Level 
	At quarterly report


	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	N/A




	Substances(s) detected
	N/A

	Concentrations of substances detected
	N/A

	Date of monitoring/sampling
	N/A


Part B to be supplied as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	During November and December, waste placement was underway close to LW4 which caused disturbance to the pumping from this well. The pumps had to be disconnected to allow the pipework to be moved out of the way for Operations to continue. The leachate level in January is compliant and the pumps are running now that waste placement operations have moved away from the well.

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	See previous Schedule 5s


	Name*
	Simon Milford

	Post
	Site Manager

	Signature
	Simon Milford

	Date
	


* authorised to sign on behalf of the Operator.

