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Permit with introductory note
The Environmental Permitting (England & Wales) Regulations 2016


[bookmark: _Hlk89679228]Lloyd’s Animal Feeds (Western) Limited

Wrexham Mill
[bookmark: _Hlk89679238]Bridge Road North
Wrexham Industrial Estate
Wrexham
LL13 9PS



Permit number
[bookmark: _Hlk89679251]EPR/AB3492ZQ

Wrexham Mill
Permit number EPR/AB3492ZQ
Introductory note
This introductory note does not form a part of the permit
The main features of the permit are as follows.  
Wrexham Mill is an animal feed manufacturing facility operated by Lloyd’s Animal Feeds (Western) Limited. The mill, which has been operational since the mid 1980s, manufactures compound animal feeds. The facility can manufacture approximately 225,000 tonnes of feed per year, depending on demand. 
The site is located in Wrexham Industrial Estate, approximately 4.5 km to the east of Wrexham.  
The products manufactured in the mill are based upon core formulations of cereals (e.g. wheat, maize, barley), and other natural ingredients (e.g. soya bean meal, rapeseed meal, sunflower kernel), plus specific additives such as mineral and vitamin supplements. 
The key processes undertaken at the site are the receipt and storage of raw materials, weighing, grinding, mixing, conditioning, pressing, cooling, coating, bulk storage of the final products and dispatch from site. 
There are four emissions to air, three via cyclone abatement from press line 1, press line 2 and the heat-treated meal line cooler exhausts, and one from the 3.6 MW thermal input gas powered boiler, used for steam generation.   
All effluent from factory cleaning, boiler blowdown, vehicle washing and on site amenities goes to foul sewer. Run-off from the site buildings and yards is routed to the main surface water drain to the south of the site, that connects into the network of drains on Wrexham Industrial Site. 

There are three European Protected Sites within 10 km of the site. Midland Meres & Mosses Phase 2 RAMSAR 4.6 km away, River Dee and Bala Lake SAC 3.6 km away and Johnstown Newt Sites SAC 7.5 km away. There are no designated SSSIs within 2 km of the site. There are three designated Wildlife sites within 2 km of the site. Wrexham Industrial Estate 0.2 km away, Cefn Park 1.4 km away and Peter’s Dingle 1.6 km away.

The status log of the permit sets out the permitting history, including any changes to the permit reference number.

	[bookmark: _Hlk89679306]Status log of the permit

	Description
	Date
	Comments

	Application EPR/AB3492ZQ/A001
	Duly made 15/04/2016
	Application for an animal feed manufacturing facility

	Schedule 5 notice sent
	27/06/2016
	Further information requested from applicant

	Additional information received
	22/07/2016
	Information received in response to schedule 5

	Additional information received
	28/07/2016
	Updated site plan received in response to schedule 5

	Additional information received
	03/08/2016
	Further information received in response to schedule 5 

	Schedule 5 notice sent
	26/08/2016
	Further information requested from applicant

	Deadline for information extended
	06/10/2016
	Request for further time made by applicant

	Deadline for information extended
	24/11/2016
	Request for further time made by applicant

	Additional information received
	21/12/2016
	Information received in response to schedule 5

	Permit determined
EPR/AB3492ZQ
	17/05/2017
	Permit granted to Lloyd’s Animal Feeds (Western) Limited 

	Application received
EPR/AB3492ZQ/V002 
	Duly made 15/02/2019
	Minor technical variation for an increase in throughput from 185,000t to 225,000t

	Variation issued
EPR/AB3492ZQ/V002
	09/05/2019
	Varied and consolidated permit issued

	Regulation 61 Notice sent to operator
	27/04/2020
	Issue of a Notice under Regulation 61(1) of the EPR. Natural Resources Wales initiated review and variation to vary the permit following the publication of the revised Best Available Techniques (BAT) Reference Document (BRef) for Food, Drink and Milk.

	[bookmark: _Hlk86327330]Regulation 61 Notice Response Received
	30/10/2020
	Response to Regulation 61 Notice Received

	Additional Information Received
	[bookmark: _Hlk86327345]27/04/2021
	Additional information to the Regulation 61 Notice

	NRW initiated Variation Issued
EPR/AB3492ZQ/V003
	26/01/2022
	NRW initiated variation issued to Lloyd’s Animal Feeds (Western) Limited



End of introductory note
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Permit


The Environmental Permitting (England and Wales) Regulations 2016

Permit number 
[bookmark: _Hlk89679418]EPR/AB3492ZQ

[bookmark: OperatorName2]This is the consolidated permit referred to in the variation and consolidation notice for application EPR/AB3492ZQ/V003 authorising,

[bookmark: _Hlk89679477]Lloyd’s Animal Feeds (Western) Limited (“the operator”),
whose registered office is
[bookmark: InstallationAddress21]
[bookmark: _Hlk89679365]The Mill
Morton
Oswestry
Salop
SY10 8BH
[bookmark: _Hlk89679511]company registration number 03819415 
[bookmark: _Hlk89679524]to operate an installation at

[bookmark: _Hlk89679375]Wrexham Mill
Bridge Road North
Wrexham Industrial Estate
Wrexham
LL13 9PS
to the extent authorised by and subject to the conditions of this permit.

	Signed
	Date

	Holly Noble
	26/01/2022


Authorised on behalf of Natural Resources Wales
/
/

1	Management
1.1 General management
1.1.1 The operator shall manage and operate the activities:
(a) in accordance with a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances, closure and those drawn to the attention of the operator as a result of complaints; and
(b) using sufficient competent persons and resources.
1.1.2 Records demonstrating compliance with condition 1.1.1 shall be maintained. 
1.1.3 Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of it kept at or near the place where those duties are carried out.
1.2	Energy efficiency
1.2.1	The operator shall:
(a)	take appropriate measures to ensure that energy is used efficiently in the activities;
(b)	review and record at least every four years whether there are suitable opportunities to improve the energy efficiency of the activities; and  
(c)	take any further appropriate measures identified by a review. 
1.3	Efficient use of raw materials
1.3.1	The operator shall:
(a)	take appropriate measures to ensure that raw materials and water are used efficiently in the activities; 
(b)	maintain records of raw materials and water used in the activities;
(c)	review and record at least every four years whether there are suitable alternative materials that could reduce environmental impact or opportunities to improve the efficiency of raw material and water use; and
(d)	take any further appropriate measures identified by a review.
1.4	Avoidance, recovery and disposal of wastes produced by the activities
1.4.1 The operator shall take appropriate measures to ensure that:
(a)	the waste hierarchy referred to in Article 4 of the Waste Framework Directive is applied  to the generation of  waste by the activities; and
(b)	any waste generated by the activities is treated in accordance with the waste hierarchy referred to in Article 4 of the Waste Framework Directive; and
(c)	where disposal is necessary, this is undertaken in a manner which minimises its impact on the environment.
1.4.2 The operator shall review and record at least every four years whether changes to those measures should be made and take any further appropriate measures identified by a review.
2	Operations
2.1	Permitted activities
2.1.1	The operator is only authorised to carry out the activities specified in schedule 1 table S1.1 (the “activities”). 
2.2	The site 
2.2.1	The activities shall not extend beyond the site, being the land shown edged in green on the site plan at schedule 7 to this permit.
2.3	Operating techniques
2.3.1	(a) 	The activities shall, subject to the conditions of this permit, be operated using the 
		techniques and in the manner described in the documentation specified in 	schedule 1, table S1.2, unless otherwise agreed in writing by Natural Resources Wales.		
(b)	If notified by Natural Resources Wales that the activities are giving rise to pollution, the operator shall submit to Natural Resources Wales for approval within the period specified, a revision of any plan or other documentation (“plan”) specified in schedule 1, table S1.2 or otherwise required under this permit which identifies and minimises the risks of pollution relevant to that plan , and shall implement the approved revised plan in place of the original from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
2.3.2	Any raw materials or fuels listed in schedule 2 table S2.1 shall conform to the specifications set out in that table.
2.3.3	The operator shall ensure that where waste produced by the activities is sent to a relevant waste operation, that operation is provided with the following information, prior to the receipt of the waste:
	(a)	the nature of the process producing the waste;
	(b)	the composition of the waste;
	(c)	the handling requirements of the waste;
	(d)	the hazardous property associated with the waste, if applicable; and
	(e)	the waste code of the waste.
2.3.4	The operator shall ensure that where waste produced by the activities is sent to a landfill site, it meets the waste acceptance criteria for that landfill.
2.4	Improvement programme
2.4.1 	The operator shall complete the improvements specified in schedule 1 table S1.3 by the date specified in that table unless otherwise agreed in writing by Natural Resources Wales.
2.4.2	Except in the case of an improvement which consists only of a submission to Natural Resources Wales, the operator shall notify Natural Resources Wales within 14 days of completion of each improvement.
3	Emissions and monitoring
3.1	Emissions to water, air or land
3.1.1	There shall be no point source emissions to water, air or land except from the sources and emission points listed in schedule 3 tables S3.1, S3.2 and S3.3.
3.1.2	The limits given in schedule 3 shall not be exceeded.
3.1.3 Periodic monitoring shall be carried out at least once every 5 years for groundwater and 10 years for soil, unless such monitoring is based on a systematic appraisal of the risk of contamination.
3.2 Emissions of substances not controlled by emission limits
3.2.1 Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.
3.2.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution, submit to Natural Resources Wales for approval within the period specified, an emissions management plan which identifies and minimises the risks of pollution from emissions of substances not controlled by emission limits;
(b)	implement the approved emissions management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.2.3	All liquids in containers, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the operator has used other appropriate measures to prevent or where that is not practicable, to minimise, leakage and spillage from the primary container.
[bookmark: _Toc449070323]3.3	Monitoring 
3.3.1	The operator shall, unless otherwise agreed in writing by Natural Resources Wales, undertake the monitoring specified in the following tables in schedule 3 to this permit:
(a) point source emissions specified in table S3.1, S3.2 and S3.3		
3.3.2	The operator shall maintain records of all monitoring required by this permit including records of the taking and analysis of samples, instrument measurements (periodic and continual), calibrations, examinations, tests and surveys and any assessment or evaluation made on the basis of such data.
3.3.3	Monitoring equipment, techniques, personnel and organisations employed for the emissions monitoring programme specified in condition 3.3.1 shall have either MCERTS certification or MCERTS accreditation (as appropriate), where available, unless otherwise agreed in writing by Natural Resources Wales.
3.3.4	Permanent means of access shall be provided to enable sampling/monitoring to be carried out in relation to the emission points specified in schedule 3 tables S3.1 unless otherwise agreed in writing by Natural Resources Wales.
3.4	Odour
3.4.1	Emissions from the activities shall be free from odour at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved odour management plan, to prevent or where that is not practicable to minimise the odour. 
3.4.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to odour, submit to Natural Resources Wales for approval within the period specified, an odour management plan which identifies and minimises the  risks of pollution from odour;
(b)	implement the approved odour management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.5	Noise and vibration
3.5.1	Emissions from the activities shall be free from noise and vibration at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved noise and vibration management plan to prevent or where that is not practicable to minimise the noise and vibration.
3.5.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to noise and vibration, submit to Natural Resources Wales for approval within the period specified, a noise and vibration management plan which identifies and minimises the risks of pollution from noise and vibration;
(b)	implement the approved noise and vibration management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.6	Pests
3.6.1 	The activities shall not give rise to the presence of pests which are likely to cause pollution, hazard or annoyance outside the boundary of the site. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved pests management plan, have been taken to prevent or where that is not practicable, to minimise the presence of pests on the site.  

3.6.2 	The operator shall:             
(a)           if notified by Natural Resources Wales, submit to Natural Resources Wales for approval within the period specified, a pests management plan which identifies and minimises risks of pollution, hazard or annoyance  from pests;
(b) 	implement the pests management plan, from the date of approval, unless otherwise agreed in writing by Natural resources Wales
[bookmark: _Toc77056949][bookmark: _Toc457192259]4	Information
4.1	Records
4.1.1 All records required to be made by this permit shall:
(a) be legible;
(b) be made as soon as reasonably practicable;
(c) if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
(d) be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made, or in the case of the following records until permit surrender:
(i) off-site environmental effects; and
(ii) matters which affect the condition of the land and groundwater.
4.1.2	The operator shall keep on site all records, plans and the management system required to be maintained by this permit, unless otherwise agreed in writing by Natural Resources Wales. 
4.2	Reporting
4.2.1	The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
4.2.2	A report or reports on the performance of the activities over the previous year shall be submitted to Natural Resources Wales by 31 January (or other date agreed in writing by Natural Resources Wales) each year.  The report(s) shall include as a minimum:
(a)	a review of the results of the monitoring and assessment carried out in accordance with the permit including an interpretive review of that data; 
(b)	the annual production /treatment data set out in schedule 4 table S4.2; and
(c)	the performance parameters set out in schedule 4 table S4.3 using the forms specified in table S4.4 of that schedule.
4.2.3	Within 28 days of the end of the reporting period the operator shall, unless otherwise agreed in writing by Natural Resources Wales, submit reports of the monitoring and assessment carried out in accordance with the conditions of this permit, as follows:
(a)	in respect of the parameters and emission points specified in schedule 4 table S4.1;
(b)	for the reporting periods specified in schedule 4 table S4.1 and using the forms specified in schedule 4 table S4.4 ; and
(c)	giving the information from such results and assessments as may be required by the forms specified in those tables.
4.2.4	The operator shall, unless notice under this condition has been served within the preceding four years, submit to Natural Resources Wales, within six months of receipt of a written notice, a report assessing whether there are other appropriate measures that could be taken to prevent, or where that is not practicable, to minimise pollution.
4.3	Notifications
4.3.1	(a)	In the event that the operation of the activities gives rise to an incident or accident which significantly affects or may significantly affect the environment, the operator must immediately—
(i)	inform Natural Resources Wales, 
(ii)	take the measures necessary to limit the environmental consequences of such an incident or accident, and
(iii)	take the measures necessary to prevent further possible incidents or accidents;
(b)	in the event of a breach of any permit condition the operator must immediately—
(i)	inform Natural Resources Wales, and
(ii)	take the measures necessary to ensure that compliance is restored within the shortest possible time;
(c)	in the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment, the operator must immediately suspend the operation of the activities or the relevant part of it until compliance with the permit conditions has been restored.
4.3.2	Any information provided under condition 4.3.1(a)(i), or 4.3.1 (b)(i) where the information relates to the breach of a limit specified in the permit, shall be confirmed by sending the information listed in schedule 5 to this permit within the time period specified in that  schedule.
4.3.3	Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.
4.3.4	Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules: 
Where the operator is a registered company:
(a) any change in the operator’s trading name, registered name or registered office address; and
(b)	any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and
(b) any steps taken with a view to the dissolution of the operator.
4.3.5	Where the operator proposes to make a change in the nature or functioning, or an extension of the activities, which may have consequences for the environment and the change is not otherwise the subject of an application for approval under the Regulations or this permit:
(a) Natural Resources Wales shall be notified at least 14 days before making the change; and
(b) the notification shall contain a description of the proposed change in operation.
4.3.6	Natural Resources Wales shall be given at least 14 days notice before implementation of any part of the site closure plan.
4.3.7	Where the operator has entered into a climate change agreement with the Government, Natural Resources Wales shall be notified within one month of:
(a)	a decision by the Secretary of State not to re-certify the agreement;
(b)	a decision by either the operator or the Secretary of State to terminate the agreement; and
(c)	any subsequent decision by the Secretary of State to re-certify such an agreement. 
 4.4	Interpretation
4.4.1	In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
4.4.2	In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “without delay”, in which case it may be provided by telephone. 
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Schedule 1 - Operations 
	Table S1.1 activities

	Activity reference 
	Activity listed in Schedule 1 of the EP Regulations 
	Description of specified activity 
	Limits of specified activity 

	[bookmark: _Hlk1725878]A1
	S6.8 Part A (1)(d)(ii)
Treatment and processing of vegetable raw materials whether previously processed or unprocessed, intended for the production of feed with a finished product production capacity greater than 300 tonnes per day.
	Production of animal feeds
	From receipt of raw materials to dispatch of final product. 

Maximum of 225,000 tonnes of feed per annum. 

	Directly Associated Activity

	A2
	Steam generation
	3.6 MWth gas-fired boiler
	From receipt of fuel to emission of combustion gases.

	A3
	Storage and handling 
of raw materials
	Material intakes, silos, bulk tanks and warehousing serving the main activity.
	From receipt of materials to use in product.

	A4
	Storage of finished product
	Product bins, despatch bays and bagging plant serving the main activity.
	From the end of the production process to dispatch from site. 



	Table S1.2 Operating techniques

	Description
	Parts
	Date Received

	Process Description
	All 
	08/03/16

	Response to Schedule 5
	Part 1 emissions to air, Part 4 site drainage 
	22/07/16

	Process Steps Flow Diagram
	All
	03/05/19

	How To Comply With Your Environmental Permit
	-
	-

	Additional guidance for the Food and Drink Sector EPR 6.10
	-
	-

	Food Drink and Milk Industries BREF 2006
	-
	-

	Response to regulation 61(1) Notice – request for information dated 27/04/2020 detailing how the Operator will comply with the BAT conclusions for The Food, Drink and Milk Industries under Directive 2010/75/EU of the European Parliament and of the Council
	All
	30/10/2020 and 27/04/2021

	Further information received via E-mail
	All
	29/10/2021



	[bookmark: _Hlk88642649]Table S1.3 Improvement programme requirements

	Reference
	Requirement
	Date

	IC1
	The Operator shall submit to Natural Resources Wales an updated written procedure(s) describing how they intend to meet the following BAT requirements in accordance with requirements specified within:
· BAT Conclusion 14 of the Food, Drink and Milk Industries BRef Document (EU 2019) – Techniques to prevent, or where not practicable reduce noise and vibration emissions
	4 June 2023 or otherwise agreed in writing with Natural Resources Wales

	IC2
	The Operator shall submit to Natural Resources Wales an updated written procedure(s) describing how they intend to meet the following BAT requirements in accordance with requirements specified within:
· BAT Conclusion 7 of the Food, Drink and Milk Industries BRef Document (EU 2019) - Water consumption and wastewater discharge
	4 June 2023 or otherwise agreed in writing with Natural Resources Wales

	IC3
	The Operator shall submit to Natural Resources Wales an updated written procedure(s) describing how they intend to meet the following BAT requirements in accordance with requirements specified within:
· BAT Conclusion 2 of the Food, Drink and Milk Industries BRef Document (EU 2019)- Establish and maintain a wastewater and waste gas inventory as part of the EMS
	4 June 2023 or otherwise agreed in writing with Natural Resources Wales


Schedule 2 - Waste types, raw materials and fuels

	Table S2.1 Raw materials and fuels
	

	Raw materials and fuel description 
	Specification

	None specified
	-
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Schedule 3(a) –Emissions and monitoring effective until 3 December 2023
	Table S3.1  Point source emissions to air – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter
	Limit (including unit) 
	Reference period
	Monitoring frequency
	Monitoring standard or method

	A1 (Point A1 on Site layout in schedule 7)
	Cooler exhaust 1
	Total Particulate
	30 mg/m3
	Hourly average
	Annual
	BS EN 13284-1

	A2 (Point A2 on Site layout in schedule 7)
	Cooler exhaust 2
	Total Particulate
	30 mg/m3
	Hourly average
	Annual
	BS EN 13284-1

	A3 (Point A3 on Site layout in schedule 7)
	Cooler exhaust 3
	Total Particulate
	30 mg/m3
	Hourly average
	Annual
	BS EN 13284-1

	A4 (Point A4 on Site layout in schedule 7)
	Boiler emission exhaust
	No parameters set
	No limit set
	--
	--
	-



	Table S3.2 Point Source emissions to water (other than sewer) and land – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter  
	Limit (incl. unit)
	Reference Period
	Monitoring frequency
	Monitoring standard or method

	W1 surface water drain connecting to drain on Wrexham Industrial Estate 
	Uncontaminated rain water from roof and yard areas
	No parameters set
	No limit set
	-
	-
	-



	Table S3.3 Point source emissions to sewer, effluent treatment plant or  other transfers off-site– emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter  
	Limit (incl. Unit)
	Reference period
	Monitoring frequency
	Monitoring standard or method

	S1 [Point S1 on drawing 003] emission to foul sewer
	Boiler blowdown 
	No parameters set
	No limit set
	-
	-
	-

	S2 [Point S2 on drawing 003] emission to foul sewer
	Lorry wash
	No parameters set 
	No limit set
	-
	-
	-


Schedule 3(b) – Emissions and monitoring effective from 4 December 2023
	Table S3.1  Point source emissions to air – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter
	Limit (including unit) 
	Reference period
	Monitoring frequency
	Monitoring standard or method

	A1 (Point A1 on drawing 003)
	Cooler exhaust 1
	Total Particulate
	20 mg/Nm3 Note 1
	Periodic
	Annual
	BS EN 13284-1

	A2 (Point A2 on drawing 003)
	Cooler exhaust 2
	Total Particulate
	20 mg/Nm3 Note 1
	Periodic
	Annual
	BS EN 13284-1

	A3 (Point A3 on drawing 003)
	Cooler exhaust 3
	Total Particulate
	20 mg/Nm3 Note 1
	Periodic
	Annual
	BS EN 13284-1

	A4 (Point A4 on drawing 003)
	Boiler emission exhaust
	No parameters set
	No limit set
	--
	--
	-



Note 1: Emission limit value expressed as mass of emitted substances per volume of waste gas under the following conditions: dry gas at a temperature of 273.15 K and a pressure of 101.3 kPa without correction for oxygen content.

	Table S3.2 Point Source emissions to water (other than sewer) and land – emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter  
	Limit (incl. unit)
	Reference Period
	Monitoring frequency
	Monitoring standard or method

	W1 surface water drain connecting to drain on Wrexham Industrial Estate 
	Uncontaminated rain water from roof and yard areas
	No parameters set
	No limit set
	-
	-
	-



	Table S3.3 Point source emissions to sewer, effluent treatment plant or  other transfers off-site– emission limits and monitoring requirements

	Emission point ref. & location
	Source
	Parameter  
	Limit (incl. Unit)
	Reference period
	Monitoring frequency
	Monitoring standard or method

	S1 [Point S1 on drawing 003] emission to foul sewer
	Boiler blowdown 
	No parameters set
	No limit set
	-
	-
	-

	S2 [Point S2 on drawing 003] emission to foul sewer
	Lorry wash
	No parameters set 
	No limit set
	-
	-
	-






Schedule 4(a) - Reporting effective until 3 December 2023
Parameters, for which reports shall be made, in accordance with conditions of this permit, are listed below.
	Table S4.1 Reporting of monitoring data

	Parameter
	Emission or monitoring point/reference
	Reporting period
	Period begins

	Emissions to air
Parameters as required by condition 3.3.1
	A1, A2, A3
	Annual
	1 January



	Table S4.2: Annual production/treatment
	

	Parameter 
	Units 

	Animal Feed
	tonnes



	Table S4.3 Performance parameters

	Parameter
	Frequency of assessment
	Units

	Water usage
	Annually
	tonnes

	Energy usage
	Annually
	MWh

	Total raw material used 
	Annually
	tonnes



	Table S4.4 Reporting forms

	Media/parameter
	Reporting format
	Date of form

	Air
	Form air 1 or other form as agreed in writing by Natural Resources Wales 
	17/05/17

	Water usage
	Form water usage 1 or other form as agreed in writing by Natural Resources Wales
	17/05/17

	Energy usage
	Form energy 1 or other form as agreed in writing by Natural Resources Wales
	17/05/17

	Other performance indicators
	Form performance 1 or other form as agreed in writing by Natural Resources Wales
	17/05/17


Schedule 4(b) - Reporting effective from 4 December 2023
Parameters, for which reports shall be made, in accordance with conditions of this permit, are listed below.

	Table S4.1 Reporting of monitoring data

	Parameter
	Emission or monitoring point/reference
	Reporting period
	Period begins

	Emissions to air
Parameters as required by condition 3.3.1.
	A1, A2, A3
	Annual
	1 January



	Table S4.2: Annual production/treatment
	

	Parameter 
	Units 

	Animal Feed
	tonnes



	Table S4.3 Performance parameters

	Parameter
	Frequency of assessment
	Units

	Water usage
	Annually
	tonnes

	Energy usage
	Annually
	MWh

	Total raw material used 
	Annually
	tonnes



	Table S4.4 Reporting forms

	Media/parameter
	Reporting format
	Date of form

	Air
	Form air 1 or other form as agreed in writing by Natural Resources Wales 
	04/12/23

	Water usage
	Form water usage 1 or other form as agreed in writing by Natural Resources Wales
	17/05/17

	Energy usage
	Form energy 1 or other form as agreed in writing by Natural Resources Wales
	17/05/17

	Other performance indicators
	Form performance 1 or other form as agreed in writing by Natural Resources Wales
	17/05/17




Schedule 5 - Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A 
	Permit Number
	

	Name of operator
	

	Location of Facility
	

	Time and date of the detection 
	



	(a) Notification requirements for any activity that gives rise to an incident or accident which significantly affects or may significantly affect the environment

	To be notified within 24 hours of detection

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



	(b) Notification requirements for the breach of a permit condition

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	




	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	



	(c) In the event of a breach of permit condition which poses an immediate danger to human health or threatens to cause an immediate significant adverse effect on the environment:

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	



Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator








Schedule 6 - Interpretation 
 “accident” means an accident that may result in pollution.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“authorised officer” means any person authorised by Natural Resources Wales under section 108(1) of The Environment Act 1995 to exercise, in accordance with the terms of any such authorisation, any power specified in section 108(4) of that Act.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.675 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the activities, either from the emission points specified in schedule 3 or from other localised or diffuse sources, which are not controlled by an emission limit..
“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.
“Industrial Emissions Directive” means DIRECTIVE 2010/75/EU OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 24 November 2010 on industrial emissions
“MCERTS” means the Environment Agency’s Monitoring Certification Scheme.
Pests” means Birds, Vermin and Insects.
Where a minimum limit is set for any emission parameter, for example pH, reference to exceeding the limit shall mean that the parameter shall not be less than that limit.
Unless otherwise stated, any references in this permit to concentrations of substances in emissions into air means:
(a) in relation to emissions from combustion processes, the concentration in dry air at a temperature of 273K, at a pressure of 101.3 kPa and with an oxygen content of 3% dry for liquid and gaseous fuels, 6% dry for solid fuels; and/or
(b) in relation to emissions from non-combustion sources, the concentration at a temperature of 273K and at a pressure of 101.3 kPa, with no correction for water vapour content.

Schedule 7 - Site plan
[image: ]

© Crown Copyright and database right 2017. Ordnance Survey licence number 100019741.













[image: ]Site Layout Plan –  new warehouse, silos and new outload bins shaded in red
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