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FIRE PREVENTION PLAN
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	Fire hazard
	Source of ignition
	Risk receptor/s
	Fire risk minimisation measures
	Fire risk ongoing prevention measures
	Review frequency
	Review by whom

	1
	Storage of aerosols (Non -Hazardous)
	Pressurised  containers
	· General public

· Site Staff

· Contractors
	Non -hazardous aerosols (inc.pressurised containers) to 

Hazardous aerosols to be stored in UN approved 205L  

vented drums with secure lids

All drums to be  located at least 6m

away from other

combustible materials on site


	Steel / aluminium colellections made on a regular basis not to exceed permitted waste acceptance levels (Site waste returns to be monitored)

Storage reviewed daily by site charge hand

Correct fire extinguishers available on site and all site operatives trained in their use
	Daily
	Site charge hand

	2
	Overheating / faulty small domestic appliances in site offices (including phone chargers, fridges, telephones, light bulbs and heating pipes)
	Electrical faults (Including exposed electrical wiring and lighting)
	· Site Staff

· Contractors
	All new electrical appliances to be PAT tested by competent electrician prior to use 

Cabin signage in place to increase staff awareness

Correct fire extinguishers available on site
	PAT Testing certification renewed every 2 years in line with The Electricity at Work Regulations 1989.

Electrical appliances in the site cabin are checked weekly by nominated Recycling Officer (Danielle Richards)
	Daily

Weekly
	Site chargehand

Recycling Officer (Danielle Richards)

	5
	Arson / Vandalism
	Combustible materials 
	· General public

· Site Staff

· Contractors
	Palisade fencing around site perimeter to deter routers

Anti vandal paint on tops of perimeter fences

Onwatch Security CCTV live recording during night hours

Perimeter warning signage in place to deter

Flammable materials to be located away from known site entry points
	Increased CCTV monitoring during the night by contractor (Onwatch Security LTD)

Regular meetings with North Wales Fire and Rescue Services – Arson Team for localised area updates on anti social behaviour/targeted attacks.


	Daily / As required

Monthly


	Site chargehand

Recycling Officer (Danielle Richards)



	6
	Plant / Equipment failure
	Faulty/exposed electrics

Fuel/oil leaks
	· General public

· Site Staff

· Contractors
	Daily vehicle defect checklists completed by operators
Weekly checklists completed by site staff
	Plant / Machinery preventative maintenance contracts in place to ensure health and safety compliance

Safety inspections carried out monthly

Correct fire extinguisher available on site and all site operatives trained in their use
	Daily

Monthly
	Site charge hand

Compliance Team

	7
	Hot Works (On site Welding)
	Sparks from welding
	· General public

· Site Staff

· Contractors
	Permits to work received prior to work commencing

Risk assessment carried out prior to work taking place on site
Public access restrictions put into place on site as and when required
	Risk assessments updated as soon as a change in work activity has been identified

Correct fire extinguisher available on site and all site operatives trained in their use
	Monthly / as required
	Compliance Team

	8
	Storage of chemicals
	Self Combustion due to the oxidation of mixed chemicals

Adverse chemical reactions from incompatible chemicals
	· General public

· Site Staff

· Contractors
	Chemicals stored in secure Chemsafe/ Flambank which is locked at all times

Site signage in place
	Maintain public restrictions to Chemsafe / Flambank

Chemsafes / Flambanks are emptied when the site is closed to reduce the risk of public contact with it’s contents

Chemsafes/ Flambanks are emptied regularly to avoid on site capacity issues  whilst not exceeding permitted waste acceptance levels (Site waste returns to be monitored)
	Daily

Weekly

Daily


	Site charge hand

Recycling Officer (Danielle Richards)

Site charge hand



	9
	Industrial heating equipment
	Electrical faults (Including exposed electrical wiring and lighting)
	· Site Staff

· Contractors
	All new electrical appliances to be PAT tested by competent electrician prior to use 

Cabin signage in place to increase staff awareness
	PAT Testing certification renewed every 2 years in line with The Electricity at Work Regulations 1989

Correct fire extinguisher available on site and all site operatives trained in their use
	Daily

Weekly
	Site Charge hand

Recycling Officer (Danielle Richards)

	10
	Discarded hot loads / smoking materials
	Heat generated within material
	· General public

· Site Staff

· Contractors
	Meet and greet in line with waste acceptance procedure to ensure that materials are within permit limitations

Warning signage in place around site to increase awareness
	Regular / ongoing toolbox talks for all site staff to ensure compliance with corporate waste acceptance procedure

Correct fire extinguisher available on site and all site operatives trained in their use
	Daily
	Site charge hand



	11
	Discarded smoking materials
	Naked flame around combustible/flammable materials 
	· General public

· Site Staff

· Contractors
	Site signage in place to reinforce No Smoking Policy

Smoking point for staff located outside the site boundary
	Enforcement of Flintshire’s No Smoking Policy through regular / ongoing toolbox talks

Correct fire extinguisher available on site and all site operatives trained in their use
	Daily
	Site charge hand



	
	Combustible material storage
	Self-Combustion of material
	· General public

· Site Staff

· Contractors
	All materials stored in separate receptacles to avoid cross contamination

All materials are collected separately to avoid cross contamination 

Not exceeding permitted waste acceptance tonnages
	Site waste returns to be monitored to ensure compliance with the sites environmental permit

Combustible materials are stored for a period not exceeding three months in line with NRW guidelines

Correct fire extinguisher available on site and all site operatives trained in their use
	Daily

Weekly
	Site charge hand

Recycling Officer (Danielle Richards)


Fire evacuation Procedure
Charge hand / Site attendants Responsibilities 
If a fire is discovered on site, it is the charge hand/site attendant’s responsibility to:
1. Operate a fire alarm call immediately using loud haler as located in site cabin

2. Without taking personal risk, telephone 999 from the nearest SAFE telephone and give the exact location of the fire and source of ignition if known
3. Leave the site by the nearest available exit

On hearing the fire alarm call, charge hands and site attendants should:
1. Evacuate immediately using the nearest unaffected escape, and proceed quickly and calmly to the assembly area: CASTLE PARK JUNCTION (Directly opposite the site as in map B – appendix 2)
2. Ensure visitors are escorted to the fire assembly point (as above and detailed in map B appendix 2)
3. Remain at the assembly point (map B, appendix 2) until given the all clear by the Fire Service
4. Make contact with the Operations Monitoring Officers and nominated Recycling Officer (Danielle Richards) to report the fire when it is safe to do so.
Under no circumstances must staff:
· Use fire extinguishers unless trained how to use them correctly
· Stop / return to the site cabin to collect personal belongings
· Re-enter the site until the Fire Service has deemed the site safe and the all clear has been given.
This information is detailed on the Fire Action Sign located in the site cabin
Fire Risk Assessments

Fire risk assessment checks (Example in appendix 4) are carried out on an annual basis (or if a change in work activity on site has been identified) by a technically competent nominated officer



Fire Extinguisher Identification


Fire Extinguisher Identification
	Extinguisher
	Type of Fire

	Colour
	Type
	Solids
(wood, paper, cloth) [image: image2.jpg]



	Flammable
Liquids
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	Flammable
Gasses
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	Electrical
Equipment
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	Cooking
Oils & Fats
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	Notes
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	Water
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Yes
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No
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No
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No
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No
	Dangerous if used on 'liquid fires' or electrical items
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	Foam
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Yes
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Yes
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No
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No
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Yes
	Not practical for home use.
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	Dry Powder
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Yes
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Yes
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Yes
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Yes
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No
	Safe use up to 1000v
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	 CO2
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No
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Yes
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No
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Yes
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Yes
	Safe on all voltages


Sensitive receptors within a 1KM radius of the site 
(See map B for radial map of site)

	Receptor
	Nature of site
	Impact (H&S / Environmental)
	Reportable to

	
	
	Potential pollution of nearby water course with firewater.
Air pollution caused by the combustion of materials on site causing noxious gases to be release which may cause harm to flora and fauna across the Ramsar Site.
	Natural Resources Wales (NRW) 

Buckley Fire and Rescue Services

	Castle Park
	Woodland area
	Potential spread of fire into woodland area in dry summer months leading to habitat loss.
Air pollution caused by the combustion of materials on site causing noxious gases to be release which may cause harm to human health.
	Natural Resources Wales (NRW)
Buckley Fire and Rescue Services

	Buckley Town
	Residential area
	Air pollution caused by the combustion of materials on site causing noxious gases to be release which may cause harm to human health
	Local Authority (Flintshire County Council)
Buckley Fire and Rescue Services

	A55
	Main access road through County
	Air pollution caused by the combustion of materials on site causing noxious gases to be release which may cause harm to human health
	Trunk Road Agency and Local Authority 
(Flintshire County Council)

	Railway Line
	Railway connecting line to Chester City
	Potential spread of flames to cause line-side fires leading to habitat loss and Air pollution caused by the combustion of materials on site causing noxious gases to be release which may cause harm to human health
	Network Rail and Flint Fire and Rescue Services


Appendices
1. Map A – Office Floor Plan
i) Map A b – Site Plan

2. Map B – A plan to show the location of the fire assembly point
3. Map C – A plan to show a 1KM radius of Standard Road Waste Transfer Station site
4. Example Fire Risk Assessment Checklist 

Map A - Site Plan – Standard Road Transfer Station
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Fire Action





If You Discover a Fire:





Operate the nearest fire alarm call point immediately using the loud hailer located in the site cabin


Without taking personal risk, telephone 999 from the nearest SAFE telephone and give location of fire


Leave the building by the nearest available exit





On hearing the fire alarm:


Evacuate immediately using the nearest unaffected escape route, and proceed quickly and calmly to the assembly area


CASTLE PARK JUNCTION


(Directly opposite the site)


Ensure visitors are escorted to the assembly point


Remain at your assembly point until the all clear is given








DO NOT USE FIRE EXTINGUISHERS UNLESS TRAINED


DO NOT STOP TO COLLECT PERSONAL BELONGINGS


DO NOT TAKE PERSONAL RISKS


DO NOT RE-ENTER THE BUILDING UNTIL THE ALL CLEAR IS GIVEN








Standard Road Waste Transfer Station – Fire Prevention Plan 2017
Standard Road Waste Transfer Station – Fire Prevention Plan 2017

