	[image: image1.png]Cyfoeth
Naturiol
Cymru

Natural
Resources
Wales




	EPR Compliance Assessment Report
	Report ID: 34013/0248523

 


	This form will report compliance with your permit as determined by an NRW officer

	Site
	Brisco Waste Disposal Ltd
	Permit Ref
	34013

	Operator/ Permit holder
	Brisco Waste Disposal Ltd
	

	Date
	16/09/2015 
	Time in
	10:15
	Out
	11:30

	What parts of the permit were assessed
	A, B, C, D, F

	Assessment
	Site Inspection
	EPR Activity:
	Installation
	
	Waste Op
	X
	Water Discharge
	

	Recipient’s name/position
	Shaun O'Kelly & Nick O'Kelly

	Officer’s name
	Sally Wakeford, Anwaar Younis
	Date issued
	21/09/2015


	Section 1 - Compliance Assessment Summary

	This is based on the requirements of the permit under the Environmental Permitting Regulations.  A detailed explanation and any action you may need to take are given in the “Detailed Assessment of Compliance” (section 3).  This summary details where we believe any non-compliance with the permit has occurred, the relevant condition and how the non-compliance has been categorised using our Compliance Classification Scheme (CCS).  CCS scores can be consolidated or suspended, where appropriate, to reflect the impact of some non-compliances more accurately.  For more details of our CCS scheme, contact your local office.

	Permit Conditions and Compliance Summary                    
	Condition(s) breached

	a) Permitted activities 
	1. Specified by permit
	A
	
	

	b) Infrastructure
	1.
Engineering for prevention & control of pollution
	C3
	
	2.1.2 & Table 2.1

	
	2. Closure & decommissioning
	NA
	
	

	
	3.
Site drainage engineering (clean & foul)
	A
	
	

	
	4. Containment of stored materials
	A
	
	

	
	5. Plant and equipment
	N
	
	

	c) General management
	1. Staff competency/ training
	A
	
	

	
	2. Management system & operating procedures
	C3
	
	1.1.1 & 2.1.2 Table 2.1 f)i)

	
	3. Materials acceptance
	C4
	
	1.2.1 (Table 1.2 & Working Plan)

	
	4. Storage handling, labelling, segregation
	C4
	
	1.1.1 (a) Table 1.1

	d) Incident  management
	1. Site security
	A
	
	

	
	2. Accident, emergency & incident planning
	A
	
	

	e) Emissions

	1. Air
	N
	
	

	
	2. Land & Groundwater
	N
	
	

	
	3. Surface water
	N
	
	

	
	4. Sewer
	N
	
	

	
	5. Waste
	N
	
	

	f) Amenity
	1. Odour
	A
	
	

	
	2. Noise
	A
	
	

	
	3. Dust/fibres/particulates
	A
	
	

	
	4. Pests, birds & scavengers
	A
	
	

	
	5. Deposits on road
	A
	
	

	g) Monitoring and records, maintenance and reporting
	1. Monitoring of emissions & environment
	N
	
	

	
	2. Records of activity, site diary, journal & events
	N
	
	

	
	3. Maintenance records
	N
	
	

	
	4. Reporting & notification
	N
	
	

	h) Resource efficiency
	1. Efficient use of raw materials
	NA
	
	

	
	2. Energy
	NA
	
	

	KEY:  C1, C2, C3, C4 = CCS breach category ( * suspended scores are marked with an asterisk),
A = Assessed (no evidence of non-compliance), N = Not assessed, NA = Not Applicable, O = Ongoing non-compliance – not scored

	
	
	
	
	

	Number of breaches recorded 
	4
	Total compliance score

(see section 5 for scoring scheme)
	8.2


	If the Total No Breaches is greater than zero, then please see Section 3 for details of our proposed enforcement response 


	Section 2 – Compliance Assessment Report Detail

	This section contains a report of our findings and will usually include information on:

	· the part(s) of the permit that were assessed (e.g. maintenance, training, combustion plant, etc)

· where the type of assessment was ‘Data Review’ details of the report/results triggering the assessment

· any non-compliances identified 

· any non-compliances with directly applicable legislation 
· details of any multiple non-compliances 
	· information on the compliance score accrued inc. details of suspended or consolidated scores.

· details of advice given
· any other areas of concern 

· all actions requested
· any examples of good practice.

· a reference to photos taken

	This report should be clear, comprehensive, unambiguous and normally completed within 14 days of an assessment.




	Officers Sally Wakeford and Anwaar Younis were met on site and accompanied around the site by Shaun O'Kelly and Nick O'Kelly. The purpose of the visit was a routine site inspection and site handover. The weather was clear and dry. 

 

During the site inspection some breaches of the permit were noted. 

 

B1. Infrastructure - Engineering for Prevention & Control of Emissions - CAT 3 - Permit Condition 2.1.2 (Table 2.1)
 

You have been given a CAT 3 breach under the above condition because during our inspection it was observed that two sections of the impermeable pavement were broken, causing the ponding of water on the site. One of the curbstones between the weighbridge and the ramp to the top level was missing. 

 

Your permit requires The engineered site containment and drainage systems shall be designed, constructed, inspected, validated and maintained and shall be fully documented and recorded, to be fit for purpose and to meet the standards specified in Table 2.1. 
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a) Impermeable pavement, i) Areas of impermeable pavement, bunding and sills CﬂM"vmfj — - e g 1eerln9 for Prevention & Control of Emissions - CAT 3 - Permit
bunding and sills shall be constructed and maintained so as to ctesoftWord .dood .. R

prevent fluids running off the pavement and the
transmission of fluids through the pavement or
joints.

ii) Al areas of impermeable pavement shall fall
towards the drainage system to prevent ponding.

b) Sealed drainage systems i) Areas of impermeable pavement, bunding and sills
shall be consructed and maintained so as to
prevent fluids running off the pavement and the
transmission of fluids through the pavement or
joints.

ii)  Oil interceptors shall be maintained as to intercept
all liquids that run off the pavement and inspected
no less frequently than every four months. A record
kept within the site diary of the inspection date,
depth of oil and any cleaning that is undertaken.

jii)  Drain/manhole covers will be colour coded on site;

blue for surface water and red for foul drainage.

e iy You have been given a CAT 3 breach under the above condition because during our inspection
it was observed that two sections of the impermeable pavement were broken, causing the
ponding of water on the site. One of the curbstones between the weighbridge and the ramp to
Convert, the top level was missing.

Your permit requires The engineered site containment and drainage systems shall be designed,
constructed, inspected, validated and maintained and shall be fully documented and recorded, to
be fit for purpose and to meet the standards specified in Table 2.1.
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(Insert Table 2.1 part i & i, )

You are required to take the following steps to remediate/rectify the breach, by the date listed on
page 4 of this form under Actions Required.

ACTION: Complete the required maintenance of the impermeable pavement and sealed
drainage system by 1st January 2016.

C2. Management - Management Systems & Operating Procedures - CAT 3 - Permit
n 2.1.2 (Table 2.1 f)i

c) Covered buildings or roofed Where wastes are stored under roofed areas:
areas i) Roof water shall be kept separate from Con
contaminated water and other liquids and shall be

You have been given a CAT 3 breach under the above condition because during our inspection
ey 1653 it was noted that although there is a rolling plan of maintenance for the yard, there were part of
U RSO NG 22/09/20115- the pavement that had been broken, and it appeared these had been broken for some time.

Your permit requires: The engineered site containment and drainage systems shall be designed,
constructed, inspected, validated and maintained and shall be fully documented and recorded, to
be fit for purpose and to meet the standards specified in Table 2.1.
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You are required to take the following steps to remediate/rectify the breach, by the date listed on page 5 of this form under Actions Required. 

 

ACTION: Complete the required maintenance of the impermeable pavement and sealed drainage system by 1st January 2016.

[image: image3.jpg]


[image: image4.jpg]



 Areas of broken impermeable pavement.
 

C2. Management - Management Systems & Operating Procedures - CAT 3 - Permit Condition 2.1.2 (Table 2.1 f)i))
 

You have been given a CAT 3 breach under the above condition because during our inspection it was noted that although there is a rolling plan of maintenance for the yard, there were part of the pavement that had been broken, and it appeared these had been broken for some time. 

 

Your permit requires: The engineered site containment and drainage systems shall be designed, constructed, inspected, validated and maintained and shall be fully documented and recorded, to be fit for purpose and to meet the standards specified in Table 2.1. 
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iii)

Tn the event of damage or deferoration being
detected to any skip, drum or other mobile tank or
container that is causing, or is likely to cause a leak,
that skip, drum or other mobile tank or container
shall be taken out of use immediately and its
contents removed.

The inspection and any necessary maintenance of
any skips, drums and other mobile tanks and
containers shall be recorded in the site diary;

€)

Fixed bays and other fixed
containers

i)

ii)

Al fixed bays and other fixed containers used for the
storage and treatment of wastes must be
constructed and maintained to a standard that is fit
for purpose..

The inspection and any necessary maintenance of
any fixed bay and/or other fixed containers shall be
recorded in the site diary;

Inspection and maintenance
of engineered containment

Al areas of impermeable pavement, sealed

drainage systems:

a)  Shall be inspected daily, to ensure the
continuing integrity and fitness for purpose of
their construction, and the inspection and any

necessary maintenance shall be recorded in

Effective date: 12 June 2006

Environment Agency Wales « Authorisation SWW182L
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C2. Management - Management Systems & Operating Procedures - CAT 3 - Permit
Condition 2.1.2 (Table 2.1 f)i))

You have been given a CAT 3 breach under the above condition because during our inspection
it was noted that although there is a rolling plan of maintenance for the yard, there were part of
the pavement that had been broken, and it appeared these had been broken for some time.

Your permit requires: The engineered site containment and drainage systems shall be designed,
constructed, inspected, validated and maintained and shall be fully documented and recorded, to
be fit for purpose and to meet the standards specified in Table 2.1.

CAR2V1.0 Page 2 of 6

(Insert Table 2.1 part f)i))

ACTION: Ensure that the management procedures reflect the need for quick maintenance
action, the rolling plan of maintenance may need to be increased to ensure the integrity of
the impermeable pavement.

C3. Management - Materials Acceptance - CAT 4 - Permit Condition 1.2.1 (Table 1.2 &
Working Plan)

You have been given a CAT 4 breach under the above condition because during our inspection
it was noted that green waste was present in the wood waste. At the time of the inspection this
waste was not on the list of wastes which should be accepted onto site.

Your permit requires: No wastes other than those which are both categorised below in Table 1.2
and specified in details in section 1.120 of the working plan shall be accepted at the site.



 

ACTION: Ensure that the management procedures reflect the need for quick maintenance action, the rolling plan of maintenance may need to be increased to ensure the integrity of the impermeable pavement. 

 

C3. Management - Materials Acceptance - CAT 4 - Permit Condition 1.2.1 (Table 1.2 & Working Plan)
 

You have been given a CAT 4 breach under the above condition because during our inspection it was noted that green waste was present in the wood waste. At the time of the inspection this waste was not on the list of wastes which should be accepted onto site. 

 

Your permit requires: No wastes other than those which are both categorised below in Table 1.2 and specified in details in section 1.120 of the working plan shall be accepted at the site. 
 

ACTION: Cease accepting waste at the site which is not listed in the above documentation, or vary the permit to allow this waste to be accepted. (Note: this action has already been completed - the permit variation was issued on 17 September 2015).
C4. Management - Storage, Handling, Labelling & Segregation - CAT 4 - Permit Condition 1.1.1(a) Table 1.1
 

You have been given a CAT4 breach under the above condition because during out inspection it was noted that the plasterboard was escaping over the edge of the impermeable pad. 

 

Your permit requires: No waste management operations shall be authorised by this licence unless specified in and undertaken in accordance with the limitations table 1.1 of this licence. 
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ACTION: Cease accepting waste at the site which is not listed in the above
documentation, or vary the permit to allow this waste to be accepted. (Note: this action
has already been completed - the permit variation was issued on 17 September 2015).

C4. Management - Storage, Handling, Labelling & Segregation - CAT 4 - Permit Condition
1.1.1(a) Table 1

You have been given a CAT4 breach under the above condition because during out inspection it
was noted that the plasterboard was escaping over the edge of the impermeable pad.

Your permit requires: No waste management operations shall be authorised by this licence
unless specified in and undertaken in accordance with the limitations table 1.1 of this licence.

(Insert table 1.1 e)i))

ACTION: Ensure this plasterboard is stored entirely on the impermeable pad immediately.
All waste must be stored on the impermeable pavement with a sealed drainage system.

Observations/Comments

In previous inspections it has been noted that no site diary has been kept due to Shaun being on

Wakeford, Sally =
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ACTION: Ensure this plasterboard is stored entirely on the impermeable pad immediately. All waste must be stored on the impermeable pavement with a sealed drainage system. 
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Plasterboard escaping from the impermeable pavement. 

 

Observations/Comments
 

In previous inspections it has been noted that no site diary has been kept due to Shaun being on site at all times. As Nick is now completing his WAMITAB to also come online as TCM, I would like to see best practice and encourage you to start keeping a site diary. It is a requirement of your permit to complete a site diary as stated in condition 7.3. I would like to see evidence of this on my next site inspection. 

Action: maintain a site diary
 

Whilst on site you provided me with an up to date working plan. Conditions in your permit, such as 1.2.1, relate to certain parts of your working plan which was submitted in 2006. The new working plan does not have the same sections, such as WP/1.110. As the permit relates so specifically to the working plan, I must ask you to amend your new working plan to correlate with the sections in the older version. 

Action: Amend working plan sections to correlate with previous working plan. 
 

Your permit variation to allow green waste onto site has been issued in the time between the visit and the completion of this report. In your odour management plan within your working plan it mentions that there is no waste accepted on site which could cause odours. Please amend the odour management plan within your working plan to provide us with details on how this waste will be handled to avoid the potential increase in odours at your site. 

Action: Amend odour management plan within working plan for odour controls for the green waste on site. 
 

I also noted on site that there was litter, namely plastics, around the site and boundary, but not leaving site. The site is usually in a much cleaner state than it was on the day of the site inspection. Please ensure that the site is litter picked and litter remains under control to ensure no litter leaves the site.
 

Thank you for taking the time to show us around the site, and giving me an insight into the workings of the business. 
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	EPR Compliance Assessment Report
	Report ID: 34013/0248523


	This form will report compliance with your permit as determined by an NRW officer

	Site 
	Brisco Waste Disposal Ltd
	Permit
	34013

	Operator/ Permit
	Brisco Waste Disposal Ltd
	Date
	16/09/2015


	Section 3- Enforcement Response
	Only one of the boxes below should be ticked

	You must take immediate action to rectify any non-compliance and prevent repetition. 
Non-compliance with your permit conditions constitutes an offence and can result in criminal prosecutions and/or suspension or revocation of a permit.  Please read the detailed assessment in Section 2 and the steps you need to take in Section 4 below.

	Other than the provision of advice and guidance, at present we do not intend to take further enforcement action in respect of the non-compliance identified above.  This does not preclude us from taking enforcement action if further relevant information comes to light or advice isn’t followed.
	

	In respect of the above non-compliance you have been issued with a warning. At present we do not intend to take further enforcement action. This does not preclude us from taking additional enforcement action if further relevant information comes to light or offences continue.
	X

	We will now consider what enforcement action is appropriate and notify you, referencing this form.
	


	Section 4- Action(s) 

	Where non-compliance has been detected and an enforcement response has been selected above, this section summarises the steps you need to take to return to compliance and also provides timescales for this to be done.

	Criteria Ref.
	CCS Category
	Action Required/Advised 
	Due Date 

	See Section 1 above 
	
	

	B1
	C3
	Complete the required maintenance of the impermeable pavement and sealed drainage system
	01/01/2016

	C2
	C3
	Ensure that the management procedures reflect the need for quick maintenance action, the rolling plan of maintenance may need to be increased to ensure the integrity of the impermeable pavement.
	01/01/2016

	C3
	C4
	Cease accepting waste at the site which is not listed in the above documentation, or vary the permit to allow this waste to be accepted.
	01/01/2016

	C4
	C4
	Ensure this plasterboard is stored entirely on the impermeable pad immediately. All waste must be stored on the impermeable pavement with a sealed drainage system.
	N/A


	Section 5 - Compliance notes for the Operator
	
	Section 6 – General Information

	To ensure you correct actual or potential non-compliance we may
( advise on corrective actions verbally or in writing 

( require you to take specific actions in writing 

( issue a notice
( require you to review your procedures or management system
( change some of the conditions of your permit

( decide to undertake a full review of your permit
	
	Data protection notice
The information on this form will be processed by the Natural Resources Wales (NRW) to fulfill its regulatory and monitoring functions and to maintain the relevant public register(s). The NRW may also use and/or disclose it in connection with:

(  offering/providing you with its literature/services relating to environmental matters

(  consulting with the public, public bodies and other organisations (e.g. Health and Safety Executive, local authorities) on environmental issues

(  carrying out statistical analysis, research and development on environmental issues

(  providing public register information to enquirers

(  investigating possible breaches of environmental law and taking any resulting action

(  preventing breaches of environmental law

(  assessing customer service satisfaction and improving its service

(  Freedom of Information Act/Environmental Information Regulations request.

The NRW may pass it on to its agents/representatives to do these things on its behalf. You should ensure that any persons named on this form are informed of the contents of this data protection notice.

	Any breach of a permit condition is an offence and we may take legal action against you.
( We will normally provide advice and guidance to assist you to come back into compliance either after an offence is committed or where we consider that an offence is likely to be committed. This is without prejudice to any other enforcement response that we consider may be required.

( Enforcement action can include the issue of a formal caution, prosecution, the service of a notice and or suspension or revocation of the permit. 

See our Enforcement and Civil Sanctions guidance for further information
	
	

	This report does not relieve the site operator of the responsibility to 

( ensure you comply with the conditions of the permit at all times and prevent pollution of the environment
( ensure you comply with other legislative provisions which may apply.
	
	

	Non-compliance scores and categories
	
	Disclosure of information

The NRW will provide a copy of this report to the public register(s).  However, if you consider that any information contained in this report should not be released to the public register(s) on the grounds of commercial confidentiality, you must write to your local area office within twenty working days of receipt of this form indicating which information it concerns and why it should not be released, giving your reasons in full.

	CCS category
	Description
	Score
	
	

	C1
	A non-compliance which could have a  major environmental effect
	    60
	
	

	C2
	A non-compliance which could have a significant environmental effect
	31
	
	

	C3
	A non-compliance which could have a  minor environmental effect
	     4
	
	Customer charter
What can I do if I disagree with this compliance assessment report?
If you are unable to resolve the issue with your site officer, you should firstly discuss the matter with the officer’s line managers.  If you wish to raise your dispute further through our official Complaints and Commendations procedure, phone our general enquiry number  0300 065 3000 (Mon to Fri 08.00–18.00) and ask for the Customer Contact team or send an email to enquiries@naturalresourceswales.gov.uk.  If you are still dissatisfied you can make a complaint to the Public Services Ombudsman for Wales.   For advice on how to complain to the Ombudsman phone their helpline on 0845 607 0987.

	C4
	A non-compliance which has no potential environmental effect
	    0.1
	
	

	Operational Risk Appraisal (Opra) - Compliance assessment findings may affect your Opra score and/or your charges. This score influences the resource we use to assess permit compliance.
	
	

	
	
	


CAR 2 V1.0 


