Crane Cross Civic Amenity & Recycling Centre, Devonshire Drive, Saundersfoot, Pembrokeshire.
Non -Technical Summary

Pembrokeshire County Council wishes to develop a new Civic Amenity and Recycling Centre on Devonshire Drive, Saundersfoot, Pembrokeshire for residents from Tenby, Kilgetty, Saundersfoot and other surrounding areas to dispose of their waste and recycling.
The existing site currently used by local residents is at the Salterns, Tenby. However this site layout is too small to redevelop in order to meet the current demands and standards required for a Non-Hazardous and Hazardous Household Waste Amenity Site. Increasing requirements for safety, environmental protection and improved waste separation for recycling has led to existing provisions being inadequate. 
The new facility will offer increased facilities to those currently available at the Salterns i.e. furniture for recycling, car tyres and gas bottles, these facilities will also be in a more user friendly and safer layout for the visiting public.
The proposed facility has been designed using information from the HSE guidance document “Operating Civic Amenity Sites Safely”. It will consist of a split level site layout in order to segregate public from operational vehicles, and to construct ramps to facilitate the unloading of vehicles at an elevated position; alleviating the current need at the Salterns to climb steps and access platforms to deposit recyclable waste into storage containers.
 A one way traffic management system with high visibility speed retarders and speed limit signs has also been included in the design to improve customer and operative’s safety, and ease traffic flow. This will also minimize or eliminate the need to reverse. Dedicated parking areas and drop off zones will be clearly marked to reduce congestion.
A total of 7 large open topped 40 cu/yd containers and a trailer type container for white goods (LDA’s) are to be arranged in sequence to the south of the access road to encourage as much of the waste to be recycled as possible. These include wood, MDF, scrap metal and green waste. 
A canopy is located to the east of the access road which will cover containers and stillages of TV’s and monitors, car and household batteries, low energy bulbs and fluorescent tubes, cooking oil and engine oil.

Adjacent and south of the canopy will be storage containers for furniture for reuse, mattresses, furniture for reprocessing, plasterboard and small domestic appliances.

 Containers for textiles, paper, books and media, Tetrapak and cans and plastic bottles, glass bottles and rubble are also situated in this area. A drop off point for gas bottles (Propane & Butane only) is also located in this area.
On the west side of the site a compactor shed will house a number of containers such as cardboard, carpet and residual waste for landfill. 
To the south of the compactor shed, car tyres will be stored on an impermeable surface in the operations area.

To the north of the compactor shed a gas bottle storage compound will be situated.

The safety of site users will be ensured with appropriately positioned safety handrails along the edge of the perimeter wall, with information signs to direct the public away from the operational areas at the entrance to the facility and into the public areas of the site. 
The site boundary is protected by a 2.4m high steel palisade security fence supplemented by a steel framed gate at entry/exit point. During opening hours the entry/exit point will be in the full control of the site staff that will monitor vehicle movements. Whenever the site is left unmanned, the gates will be locked shut. 
The site will be protected by a CCTV system which will record activities and can be accessed remotely from our offices in Thornton Depot. Number plate recognition will also be used on site to monitor site usage.
Lighting will be used for operational usage only and will focus on the public and operational areas of the facility. In order to protect public amenity, the proposed lighting would be florescent down-lighters and positioned horizontally with no upward tilt, in order to ensure that there is no ‘glare’ or light trespass to adjoining properties.
Signage provision within the site will serve a number of purposes. Primarily, signage at the entrance to the site will provide information on what materials can be accepted, opening hours, Permit No. and out of hours contact details.

Drainage for the site will consist of two systems.
A sealed system for the foul from the site toilet facilities and for any leachate coming from the compactor shed will be collected in two cesspools with a total volume of 11,000 litres.
A surface / storm water system will consist of linear kerb drains and rainwater gulleys taking water off site to an outfall at Knightson Brook via an oil separator, silt trap and a cellular storage tank. A pen stock valve is fitted to enable shutting off the system in an emergency, e.g. fire on site.
Hazardous waste storage limits are within the Industrial Emissions Directive (IED) guidelines. Procedures are in place for when capacity limits are imminent.
Local Natural Resources Wales officers have been involved during the design and planning stages of the redevelopment and are fully aware of the project.
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