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Permit with introductory note
The Environmental Permitting (England & Wales) Regulations 2016

Pic-Up Spares Limited

Pic Up Spares Ltd
Jersey Road
Winch Wen
Swansea
SA1 7DW



Permit number
EPR/AP3498FR

Pic Up Spares Ltd
Permit number EPR/AP3498FR
Introductory note
This introductory note does not form a part of the permit
The main features of the permit are as follows.  
This is a Tier 3 Bespoke permit for the recovery, treatment, storage (including temporary storage) and dismantling of waste motor vehicles for recovery and/or disposal.
All treatment of hazardous and non-hazardous waste must take place on an impermeable surface with sealed drainage.
All hazardous waste must be stored on an impermeable surface with sealed drainage.
Treatment activities permitted on site include sorting, separating, cutting, crushing, granulating, depollution and dismantling. 
The permitted treatment activities also include the treatment (de-canning) of catalytic converters. This treatment activity results in producing metal casing which has refractory ceramic fibre (RCF) matting remaining within. Due to the waste potentially containing RCF matting it is classified as hazardous waste and given a waste code of; 16 02 21*.
There will be no treatment of catalytic converters apart from the decanning process.
Relevant storage and treatment capacity thresholds have been included in the permit to reflect the legal waste facility operational limits; above which, the site would be operating as an Industrial Emissions Directive installation. (See Table S1.1 for relevant limits.)
This permit does not allow any point source emission into surface waters or groundwater except: 
- clean, rainfall dependant drainage from areas of the site not used in connection with the storage and/or treatment of waste, and
- integral discharge(s) from the permitted activity (outside areas of the site used in connection with the storage and/or treatment of waste) in accordance with the limits set out in Table S1.1.
All emissions from the activity which are not controlled via actual emission limits, are controlled through the ‘emission of substances not controlled by emission limits condition’ and any all relevant process requirements set out in Tables S1.1 and S1.2.  
The burning of any wastes, either in the open, inside buildings or in any form of incinerator is not permitted.
The status log of the permit sets out the permitting history, including any changes to the permit reference number.

	Status log of the permit

	Description
	Date
	Comments

	Licence issued (EAWML 34238)
	04/08/04
	Original waste management licence for end-of-life vehicle depollution and dismantling authorised treatment facility.

	Modification issued 
	25/04/06
	Recording of waste accepted and removed conditions – 6.1 ,6.2 included.

	Variation issued EPR/AP3498FR/V003 (formerly EAWML 34238)  
	12/06/06
	Table 2.1 (Specified end-of-life vehicle storage and treatment operations) replaced.

	Application EPR/ AP3498FR/V004
(variation and consolidation)
	Duly made
28/04/17
	Application to vary the permit to include decanning treatment activity for the catalytic converters and update the permit to modern conditions.

	Variation determined EPR/AP3498FR
	DRAFT
	Varied and consolidated permit issued in modern condition format.



End of introductory note
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Permit


The Environmental Permitting (England and Wales) Regulations 2016

Permit number 
EPR/AP3498FR
The Natural Resources Body for Wales (“Natural Resources Wales”) authorises, under regulation 13 of the Environmental Permitting (England and Wales) Regulations 2016
[bookmark: OperatorName2]
Pic-Up Spares Limited (“the operator”),

whose registered office is
[bookmark: InstallationAddress21]
44 Saint Helens Road
Swansea
SA1 4BB

company registration number 1183310 
to operate waste operations at

Pic Up Spares Ltd
Jersey Road
Winch Wen
Swansea
SA1 7DW
to the extent authorised by and subject to the conditions of this permit.

	Name
	Date

	DRAFT
	DRAFT


Authorised on behalf of Natural Resources Wales


Conditions 
1 Management
1.1 General management
1.1.1 The operator shall manage and operate the activities:
(a) in accordance with a written management system that identifies and minimises risks of pollution, including those arising from operations, maintenance, accidents, incidents, non-conformances , closure and those drawn to the attention of the operator as a result of complaints; and
(b) using sufficient competent persons and resources.
1.1.2 Records demonstrating compliance with condition 1.1.1 shall be maintained. 
1.1.3 Any person having duties that are or may be affected by the matters set out in this permit shall have convenient access to a copy of it kept at or near the place where those duties are carried out.
1.1.4 The operator shall comply with the requirements of an approved competence scheme.
Avoidance, recovery and disposal of wastes produced by the activities
1.2.1 The operator shall take appropriate measures to ensure that:
(a) the waste hierarchy referred to in Article 4 of the Waste Framework Directive is applied to the generation of waste by the activities; and
(b) any waste generated by the activities is treated in accordance with the waste hierarchy referred to in Article 4 of the Waste Framework Directive; and
(c) where disposal is necessary, this is undertaken in a manner which minimises its impact on the environment.
1.2.2 The operator shall review and record at least every four years whether changes to those measures should be made and take any further appropriate measures identified by a review.
2	Operations
2.1	Permitted activities
2.1.1	The operator is only authorised to carry out the activities specified in schedule 1 table S1.1 (the “activities”). 
2.2	The site 
2.2.1	The activities shall not extend beyond the site, being the land shown edged in green on the site plan at schedule 7 to this permit.
2.3	Operating techniques
2.3.1	(a) 	The activities shall, subject to the conditions of this permit, be operated using the 
		techniques and in the manner described in the documentation specified in 	schedule 1, table S1.2, unless otherwise agreed in writing by Natural Resources Wales.		
(b)	If notified by Natural Resources Wales that the activities are giving rise to pollution, the operator shall submit to Natural Resources Wales for approval within the period specified, a revision of any plan or other documentation (“plan”) specified in schedule 1, table S1.2 or otherwise required under this permit which identifies and minimises the risks of pollution relevant to that plan , and shall implement the approved revised plan in place of the original from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
2.3.2	Waste shall only be accepted if:
(a)	it is of a type and quantity listed in schedule 2 table(s) S2.1 [, S2.2 etc.]; and 
(b)	it conforms to the description in the documentation supplied by the producer and holder.
2.4	Technical requirements
		Vehicle depollution and dismantling

2.4.1	The storage (including temporary storage) and treatment of waste motor vehicles shall meet the requirements of article 6(1) of the End-of-Life Vehicles Directive.
		Hazardous waste storage and treatment
2.4.2	Hazardous waste shall not be mixed, either with a different category of hazardous waste or with other waste, substances or materials, unless it is authorised by schedule 1 table S1.1 and appropriate measures are taken.
2.5	Improvement programme
2.5.1 	The operator shall complete the improvements specified in schedule 1 table S1.3 by the date specified in that table unless otherwise agreed in writing by Natural Resources Wales.
2.5.2	Except in the case of an improvement which consists only of a submission to Natural Resources Wales, the operator shall notify Natural Resources Wales within 14 days of completion of each improvement.
3	Emissions and monitoring
3.1 Emissions of substances not controlled by emission limits
3.1.1 Emissions of substances not controlled by emission limits (excluding odour) shall not cause pollution. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved emissions management plan, have been taken to prevent or where that is not practicable, to minimise, those emissions.
3.1.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution, submit to Natural Resources Wales for approval within the period specified, an emissions management plan which identifies and minimises the risks of pollution from emissions of substances not controlled by emission limits;
(b)	implement the approved emissions management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.1.3	All liquids in containers, whose emission to water or land could cause pollution, shall be provided with secondary containment, unless the operator has used other appropriate measures to prevent or where that is not practicable, to minimise, leakage and spillage from the primary container.
[bookmark: _Toc449070323]3.2	Odour
3.2.1	Emissions from the activities shall be free from odour at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved odour management plan, to prevent or where that is not practicable to minimise the odour. 
3.2.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to odour, submit to Natural Resources Wales for approval within the period specified, an odour management plan which identifies and minimises the risks of pollution from odour;
(b)	implement the approved odour management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.3	Noise and vibration
3.3.1	Emissions from the activities shall be free from noise and vibration at levels likely to cause pollution outside the site, as perceived by an authorised officer of Natural Resources Wales, unless the operator has used appropriate measures, including, but not limited to, those specified in any approved noise and vibration management plan to prevent or where that is not practicable to minimise the noise and vibration.
3.3.2	The operator shall:
(a)	if notified by Natural Resources Wales that the activities are giving rise to pollution outside the site due to noise and vibration, submit to Natural Resources Wales for approval within the period specified, a noise and vibration management plan which identifies and minimises the risks of pollution from noise and vibration;
(b)	implement the approved noise and vibration management plan, from the date of approval, unless otherwise agreed in writing by Natural Resources Wales.
3.4	Pests
3.4.1 	The activities shall not give rise to the presence of pests which are likely to cause pollution, hazard or annoyance outside the boundary of the site. The operator shall not be taken to have breached this condition if appropriate measures, including, but not limited to, those specified in any approved pests management plan, have been taken to prevent or where that is not practicable, to minimise the presence of pests on the site.  

3.4.2 	The operator shall:             
(a)           if notified by Natural Resources Wales, submit to Natural Resources Wales for approval within the period specified, a pests management plan which identifies and minimises risks of pollution, hazard or annoyance from pests;
(b)           implement the pests management plan, from the date of approval, unless otherwise agreed in writing by Natural resources Wales.
3.5	Fire
3.5.1	The operator shall manage and operate the activities in accordance with a written fire prevention plan using the current, relevant fire prevention plan guidance. 
3.5.2	The operator shall:
(a) 	if notified by Natural Resources Wales that the activities could cause a fire risk, submit to Natural Resources Wales a fire prevention plan which identifies and minimises the risks of fire;
(b)	Operate the activity in accordance with the fire prevention plan, from the date of submission, unless otherwise agreed in writing by Natural Resources Wales.
[bookmark: _Toc77056949][bookmark: _Toc457192259]4	Information
4.1	Records
4.1.1 All records required to be made by this permit shall:
(a) be legible;
(b) be made as soon as reasonably practicable;
(c) if amended, be amended in such a way that the original and any subsequent amendments remain legible, or are capable of retrieval; and
(d) be retained, unless otherwise agreed in writing by Natural Resources Wales, for at least 6 years from the date when the records were made, or in the case of the following records until permit surrender:
(i) off-site environmental effects; and
(ii) matters which affect the condition of the land and groundwater.
4.1.2	The operator shall keep on site all records, plans and the management system required to be maintained by this permit, unless otherwise agreed in writing by Natural Resources Wales. 
4.2	Reporting
4.2.1	The operator shall send all reports and notifications required by the permit to Natural Resources Wales using the contact details supplied in writing by Natural Resources Wales.
4.2.2	Within one month of the end of each year, the operator shall submit to Natural Resources Wales using the form made available for the purpose, the information specified on the form relating to the site and the waste accepted and removed from it during the previous quarter.
4.3	Notifications
4.3.1	Natural Resources Wales shall be notified without delay following the detection of:
(a) any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution;
(b) the breach of a limit specified in the permit; or 
(c) any significant adverse environmental effects.  
4.3.2	Any information provided under condition 4.3.1 shall be confirmed by sending the information listed in schedule 5 to this permit within the time period specified in that schedule.
4.3.3	Where Natural Resources Wales has requested in writing that it shall be notified when the operator is to undertake monitoring and/or spot sampling, the operator shall inform Natural Resources Wales when the relevant monitoring and/or spot sampling is to take place. The operator shall provide this information to Natural Resources Wales at least 14 days before the date the monitoring is to be undertaken.
4.3.4	Natural Resources Wales shall be notified within 14 days of the occurrence of the following matters, except where such disclosure is prohibited by Stock Exchange rules: 
Where the operator is a registered company:
(a) any change in the operator’s trading name, registered name or registered office address; and
(b)	any steps taken with a view to the operator going into administration, entering into a company voluntary arrangement or being wound up.
Where the operator is a corporate body other than a registered company:
(a) any change in the operator’s name or address; and
(b) any steps taken with a view to the dissolution of the operator.
	In any other case: 
(a) the death of any of the named operators (where the operator consists of more than one named individual);
(b) any change in the operator’s name(s) or address(es); and
(c) any steps taken with a view to the operator, or any one of them, going into bankruptcy, entering into a composition or arrangement with creditors, or, in the case of them being in a partnership, dissolving the partnership.
4.3.5	Where the operator proposes to make a change in the nature or functioning, or an extension of the activities, which may have consequences for the environment and the change is not otherwise the subject of an application for approval under the Regulations or this permit:
(a) Natural Resources Wales shall be notified at least 14 days before making the change; and
(b) the notification shall contain a description of the proposed change in operation.

 4.4	Interpretation
4.4.1	In this permit the expressions listed in schedule 6 shall have the meaning given in that schedule.
4.4.2	In this permit references to reports and notifications mean written reports and notifications, except where reference is made to notification being made “without delay”, in which case it may be provided by telephone. 
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	Table S1.1 activities

	
	Description of activities for waste operations 
	Limits of activities

	A1- End-of-life vehicle storage and depollution facility 
	R13: Storage of waste pending any of the operations numbered R1 to R12 (excluding temporary storage, pending collection, on the site where it is produced)
 
R4: Recycling/reclamation of metals and metal compounds

R5: Recycling/reclamation of other inorganic compounds


	All hazardous and non-hazardous waste must be stored and treated on an impermeable surface with sealed drainage.

Uncontaminated plastic, glass and ferrous and non- ferrous metal wastes arising from the treatment of end-of-life vehicles shall be stored on hard standing or an impermeable surface with sealed drainage system.

The maximum quantity of hazardous waste that can be stored at the site in total for recovery or disposal, shall not exceed 50 tonnes at any one time.

The maximum quantity of hazardous waste treated for recovery shall not exceed 10 tonnes per day. (excluding end of life vehicles pending manual dismantling, repair or refurbishment).

Lead acid batteries shall be stored in containers with an impermeable, acid resistant base and a lid to prevent ingress of water. 

Treatment operations shall be limited to manual and/or mechanical: 
· sorting
· stripping
· segregating
· shredding
· separation
· compacting
· granulating
· crushing
· compaction
· dismantling
· decanning of the catalytic converters 
· depollution of waste motor vehicles
· bulking up for onwards transfer
of permitted waste for the purpose of recovery and/or disposal.

There shall be no treatment of:
- waste batteries and/or accumulators
- breakpads containing asbestos
- oil filters
other than bulking up for onward transfer.

Waste types as specified in Table S2.1

	Site drainage
	[bookmark: _GoBack]Drainage consisting solely of;
· clean, rainfall dependant drainage from areas of the site not used in connection with the storage and/or treatment of waste
· run-off from the impermeable surface from external areas of the site used to store and/or treat waste.

No visible oil or grease shall be present in the discharge.

There shall be no discharge from the buildings on site used to store and/or treat waste.




	Table S1.2 Operating techniques

	Description
	Parts
	Date Received

	Response to Schedule 5 Notice served on 3rd July 2017

	Operating Techniques and procedures
· Environmental Risk Assessment
· Block Plan

	25/07/2017

	
	Email dated 31st August 2017 confirming there will be no integral discharge from the site activities.
	31/08/2017

	Technical Guidance Document: ‘How to comply with your environmental permit’
	All relevant sections
	N/A

	Sector Guidance Note IPPC S5.06: Guidance for the Recovery and Disposal of Hazardous and Non Hazardous Waste
	All relevant sections
	N/A

	Fire prevention and mitigation plan guidance 
	All relevant sections
	N/A



	Table S1.3 Improvement programme requirements

	Reference
	Requirement
	Date

	IPC 1
	The operator shall submit a written Fire prevention and mitigation plan to Natural Resources Wales for approval. 
The Fire prevention and mitigation plan must be produced in line with the standards set out in the current fire prevention and mitigation plan guidance – Waste 
	3 months after permit issue or otherwise agreed in writing with Natural Resources Wales





Schedule 2 - Waste types, raw materials and fuels
	Table S2.1 Permitted waste types and quantities for end-of-life vehicle depollution and dismantling facility

	Maximum quantity
	The total quantity of waste accepted at the site shall be not exceed 5000 tonnes per year.

	Exclusions
	Notwithstanding the waste types set out in this table, wastes having any of the following characteristics shall not be accepted:
· consisting solely or mainly of dusts, powders or loose fibres



	Waste code
	Description

	13 
	OIL WASTES AND WASTES OF LIQUID FUELS (except edible oils, and those in chapters 05, 12 and 19)

	13 01 
	waste hydraulic oils

	13 01 09* 
	mineral-based chlorinated hydraulic oils

	13 01 10* 
	mineral based non-chlorinated hydraulic oils

	13 01 11* 
	synthetic hydraulic oils

	13 01 12* 
	readily biodegradable hydraulic oils

	13 01 13* 
	other hydraulic oils

	13 02 
	waste engine, gear and lubricating oils

	13 02 04*
	mineral-based chlorinated engine, gear and lubricating oils

	13 02 05* 
	mineral-based non-chlorinated engine, gear and lubricating oils

	13 02 06* 
	synthetic engine, gear and lubricating oils

	13 02 08* 
	other engine, gear and lubricating oils

	13 07 
	wastes of liquid fuels

	13 07 01*
	fuel oil and diesel

	13 07 02* 
	petrol

	13 07 03* 
	other fuels (including mixtures)

	14
	WASTE ORGANIC SOLVENTS, REFRIGERANTS AND PROPELLANTS (except 07 and 08)

	14 06 
	waste organic solvents, refrigerants and foam/aerosol propellants

	14 06 01* 
	chlorofluorocarbons, HCFC, HFC

	14 06 02* 
	other halogenated solvents and solvent mixtures

	14 06 03* 
	other solvents and solvent mixtures

	16 
	16 WASTES NOT OTHERWISE SPECIFIED IN THE LIST

	16 01
	end-of-life vehicles from different means of transport (including off-road machinery) and wastes from dismantling of end-of-life vehicles and vehicle maintenance (except 13, 14, 16 06 and 16 08)

	16 01 03 
	end-of-life tyres

	16 01 04*
	End of life vehicles

	16 01 06 
	end-of-life vehicles, containing neither liquids nor other hazardous components

	16 01 07* 
	oil filters

	16 01 08* 
	components containing mercury

	16 01 09* 
	components containing PCBs

	16 01 10* 
	explosive components (for example air bags)

	16 01 11* 
	brake pads containing asbestos

	16 01 12 
	brake pads other than those mentioned in 16 01 11

	16 01 13* 
	brake fluids

	16 01 14* 
	antifreeze fluids containing dangerous substances

	16 01 15 
	antifreeze fluids other than those mentioned in 16 01 14

	16 01 16
	tanks for liquefied gas

	16 01 17 
	ferrous metal

	16 01 18 
	non-ferrous metal

	16 01 19 
	plastic

	16 01 20 
	glass

	16 01 21* 
	hazardous components other than those mentioned in 16 01 07 to 16 01 11 and 16 01 13 and 16 01 14

	16 01 22 
	components not otherwise specified

	16 06
	batteries and accumulators

	16 06 01* 
	lead batteries

	16 06 05 
	other batteries and accumulators




Schedule 3 – Emissions and monitoring
There are no emission limits or associated monitoring requirements.










Schedule 4 - Reporting
There is no reporting under this schedule.




Schedule 5 - Notification 
These pages outline the information that the operator must provide. 
Units of measurement used in information supplied under Part A and B requirements shall be appropriate to the circumstances of the emission. Where appropriate, a comparison should be made of actual emissions and authorised emission limits.
If any information is considered commercially confidential, it should be separated from non-confidential information, supplied on a separate sheet and accompanied by an application for commercial confidentiality under the provisions of the EP Regulations.
Part A 
	Permit Number
	

	Name of operator
	

	Location of Facility
	

	Time and date of the detection 
	



	(a) Notification requirements for any malfunction, breakdown or failure of equipment or techniques, accident, or emission of a substance not controlled by an emission limit which has caused, is causing or may cause significant pollution

	To be notified within 24 hours of detection

	Date and time of the event
	

	Reference or description of the location of the event 
	

	Description of where any release into the environment took place
	

	Substances(s) potentially released
	

	Best estimate of the quantity or rate of  release of substances
	

	Measures taken, or intended to be taken, to stop any emission
	

	Description of the failure or accident.
	



	(b) Notification requirements for the breach of a limit

	To be notified within 24 hours of detection unless otherwise specified below

	Emission point reference/ source
	

	Parameter(s)
	

	Limit
	

	Measured value and uncertainty
	

	Date and time of monitoring
	

	Measures taken, or intended to be taken, to stop the emission
	




	Time periods for notification following detection of a breach of a limit

	Parameter
	Notification period

	
	

	
	

	
	



	(c) Notification requirements for the detection of any significant adverse environmental effect

	To be notified within 24 hours of detection

	Description of where the effect on the environment was detected
	

	Substances(s) detected
	

	Concentrations of substances detected
	

	Date of monitoring/sampling
	



Part B - to be submitted as soon as practicable
	Any more accurate information on the matters for notification under Part A.
	

	Measures taken, or intended to be taken, to prevent a recurrence of the incident
	

	Measures taken, or intended to be taken, to rectify, limit or prevent any pollution of the environment which has been or may be caused by the emission
	

	The dates of any unauthorised emissions from the facility in the preceding 24 months.
	



	Name*
	

	Post
	

	Signature
	

	Date
	


* authorised to sign on behalf of the operator
Schedule 6 - Interpretation 
“accident” means an accident that may result in pollution.
“Annex I” means Annex I to Directive 2008/98/EC of the European Parliament and of the Council on waste.
“Annex II” means Annex II to Directive 2008/98/EC of the European Parliament and of the Council on waste.
“application” means the application for this permit, together with any additional information supplied by the operator as part of the application and any response to a notice served under Schedule 5 to the EP Regulations.
“authorised officer” means any person authorised by Natural Resources Wales under section 108(1) of The Environment Act 1995 to exercise, in accordance with the terms of any such authorisation, any power specified in section 108(4) of that Act.
“emissions of substances not controlled by emission limits” means emissions of substances to air, water or land from the activities, either from the emission points specified in schedule 3 or from other localised or diffuse sources, which are not controlled by an emission or background concentration limit.
“End-of-Life Vehicles Directive” means Directive 2000/53/EC of the European Parliament and Council of 18 September 2000 on end-of-life vehicles.
“EP Regulations” means The Environmental Permitting (England and Wales) Regulations SI 2016 No.1154 and words and expressions used in this permit which are also used in the Regulations have the same meanings as in those Regulations.
“groundwater” means all water, which is below the surface of the ground in the saturation zone and in direct contact with the ground or subsoil.
“hazardous property” has the meaning in 8Annex lll of the Waste Framework Directive  
“hazardous substance” means a substance classified as hazardous as a consequence of fulfilling the criteria laid down in parts 2 to 5 of Annex I to Regulation (EC) No 1272/2008
“hazardous waste” has the meaning given in the Hazardous Waste (Wales) Regulations 2005 (as amended)
“impermeable surface” means a surface or pavement constructed and maintained to a standard sufficient to prevent the transmission of liquids beyond the surface.
“Pests” means Birds, Vermin and Insects.
“quarter” means a calendar year quarter commencing on 1 January, 1 April, 1 July or 1 October.
“R” means a recovery operation provided for in Annex II to Directive 2008/98/EC of the European Parliament and of the Council on waste.
“waste code” means the six digit code referable to a type of waste in accordance with the list of wastes established by Commission Decision 2000/532/EC as amended from time to time (the ‘List of Wastes Decision’) and in relation to hazardous waste, includes the asterisk.
“Waste Framework Directive” or “WFD” means Waste Framework Directive 2008/98/EC of the European Parliament and of the Council on waste.
 “year” means calendar year ending 31 December.
Schedule 7 - Site plan

This is the plan referred to in the permit.
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© Crown Copyright and database right [2017]. Ordnance Survey licence number 100019741.

END OF PERMIT
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