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	Consent no
	NRWWIA310

	
	


WATER INDUSTRY ACT 1991

SECTION 165 / 166
CONSENT TO DISCHARGE

TO:
Dwr Cymru


Linea


Fortran Road


St Mellons


Cardiff


CF3 OLT
	The NATURAL RESOURCES BODY FOR WALES ("Natural Resources Wales") in pursuance of its powers under the Water Industry Act 1991 HEREBY CONSENTS to the making of a discharge as follows:
Raw Water


	FROM: Usk Reservoir, Trecastle, Powys, LD3 8YF

	

	AT: NATIONAL GRID REFERENCE SN 83416 28932

	

	TO: River usk

	

	SUBJECT TO: the conditions set out in the following schedule:

Raw Water                     Schedule No. NRWWIA310

	

	This consent is issued on the 24th day of March 2022
This consent takes effect on the 28th day of March 2022
This consent shall cease to have effect on the 25th day of April 2022
Signed: Terry Gulliford


	


CONDITIONS OF CONSENT TO DISCHARGE

RAW WATER (“the Discharge”)

NATURE OF THE DISCHARGE

1.
The Discharge shall consist solely of raw water. 

SOURCE OF THE DISCHARGE

2. The Discharge shall be derived from Usk Reservoir.
LOCATION OF DISCHARGE

3.
The location of the Discharge shall be at NGR SN 83416 28932, marked ‘Discharge Point’ on the site plan in Annex 1.

SAMPLE POINT

4.
A sample point shall be provided and maintained so that a representative sample of the Discharge may be obtained. 

VOLUME

5. The total volume of the Discharge shall not exceed 64,800 cubic metres.

6. The total daily volume of the Discharge shall not exceed 21,600 cubic metres.

7. The rate of the Discharge shall not exceed 4,000 litres per second.
COMPOSITION

8.
The consent holder shall take all necessary steps to secure that any water discharged by it under this consent is as free as may be reasonably practicable from — 

(a) 
mud and silt;

(b) 
solid, polluting, offensive or injurious substances; 
and

(c)
any substances prejudicial to fish or spawn, or to spawning beds or food of fish.
SCOURING
9.
The rate of discharge shall be controlled to prevent any significant scouring of the bed or bankside of the receiving water. 
FLOODING

10.
The discharge shall not cause or significantly contribute to flooding in the downstream catchment.
PERIOD OF DISCHARGE

11.
The Discharge shall only be made between 28th day of March 2022 and the 25th day of April 2022.
ANNEX 1- PLAN No. NRWWIA310
[image: image1.png]3

[Overflow Spillway





© Crown Copyright and database right 2022. Ordnance Survey licence number 100019741.

