
[bookmark: _Hlk65593594]Permit Number: 	EPR/UP3237CP			Operator: 	Solway Foods Limited

Facility:		 RF Brookes				Form Number:  Air1 / 25/03/2022
Reporting of emissions to air for the period from DD/MM/YYYY to DD/MM/YYYY 
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	A1
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A1
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A1
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A2
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A2
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A2
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A3
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A3
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A3
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A4
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A4
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A4
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A5

	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A5
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A5

	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A6
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A6
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A6
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A8
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A8
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A8
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A9
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A9
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A9
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	

	A10
	[bookmark: _Hlk535568070]Oxides of Nitrogen (NO and NO2 expressed as NO2)
	95 mg/ m3
	In line with NRW TGN M5
	
	NRW TGN M5
	
	

	A10
	Carbon Monoxide
	No limit set
	In line with NRW TGN M5
	
	NRW TGN M5
	
	

	A11
	Oxides of Nitrogen (NO and NO2 expressed as NO2)
	No limit set
	Periodic
	
	EN 14792
	
	

	A11
	Carbon Monoxide
	No limit set
	Periodic
	
	EN 15058 or CEN TS 17337
	
	

	A11
	Particulates
	No limit set
	Periodic
	
	EN 13284-1
	
	






[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.


Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number:  EPR/UP3237CP			Operator: 		Solway Foods Limited

Facility: 	RF Brookes				Form Number: 	Sewer1 / 25/03/2022
Reporting of emissions to sewer for the period from DD/MM/YYYY to DD/MM/YYYY
	Emission
Point
	Substance /
Parameter
	Emission
Limit Value
	Reference Period
	Result [1]
	Test
Method [2]
	Sample
Date and Times [3]
	Uncertainty
[4]

	S1
	Effluent Flow Rate 	
	No Limit set
	Continuous
	
	As agreed in
improvement
programme number 7
	
	

	S1
	Chemical Oxygen Demand (COD)
	No Limit set
	Spot Sample
	
	BS ISO 15705:2002, BS 6068-
2.80:2002
	
	

	S1
	Suspended solids
	No Limit set
	Spot Sample
	
	BSEN872:1996,
BS6068 2.54:1996
	
	

	S1
	pH
	No Limit set
	Spot Sample
	
	BS ISO 15705:2002, BS 6068-
2.80:2002
	
	

	S1
	Cadmium and its compounds, expressed as cadmium (Total Cd)
	0.01mg/litre

	Spot Sample
	
	Mass Balance Calculation
	
	

	S1
	Mercury and its compounds, expressed as mercury (Total Hg)
	0.0001 mg/litre

	Spot Sample
	
	Mass Balance Calculation
	
	

	S1
	Cadmium and its compounds, expressed as cadmium (Total Cd)
	2800 g/year
	Spot Sample
	
	Mass Balance Calculation
	
	

	S1
	Mercury and its compounds, expressed as mercury (Total Hg)
	330 g/year
	Spot Sample
	
	Mass Balance Calculation
	
	



[1] The result given is the maximum value (or the minimum value in the case of a limit that is expressed as a minimum) obtained during the reporting period, expressed in the same terms as the emission limit value. Where the emission limit value is expressed as a range, the result is given as the ‘minimum – maximum’ measured values.
[2] Where an internationally recognised standard test method is used the reference number is given. Where another method that has been formally agreed with Natural Resources Wales is used, then the appropriate identifier is given. In other cases the principal technique is stated, for example gas chromatography.
[3] For non-continuous measurements the date and time of the sample that produced the result is given. For continuous measurements the percentage of the process operating time covered by the result is given.   
[4] The uncertainty associated with the quoted result at the 95% confidence interval, unless otherwise stated.



Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)



Permit Number: EPR/UP3237CP			Operator: 		Solway Foods Limited

Facility:	RF Brookes				Form Number: 	WaterUsage1 / 25/03/2022

Reporting of Water Usage for the year 20XX

	Water Source
	Usage
(m3/year
	Specific Usage 
(m3/unit output)
	

	
	
	
	

	
	
	
	

	Mains water
	
	
	

	Site borehole
	
	
	

	River abstraction
	
	
	

	
	
	
	

	
	
	
	

	TOTAL WATER USAGE
	
	
	



	Operator’s comments :







Signed …………………………………………………………….  		Date………………………..   	
	(authorised to sign as representative of Operator)


[bookmark: _Hlk97553347]Permit Number: EPR/UP3237CP			Operator: 		Solway Foods Limited

Facility:	RF Brookes 				Form Number: 	 Energy1 / 25/03/2022

Reporting of Energy Usage for the year 20XX

	
Energy Source
	Energy Usage
	
Specific Usage
(MWh/unit output)
	

	
	
Quantity
	Primary Energy
(MWh)
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Electricity *
	MWh
	
	
	

	Natural Gas
	MWh
	
	
	

	Gas Oil
	tonnes
	
	
	

	Recovered Fuel Oil
	tonnes
	
	
	

	
	
	
	
	

	TOTAL
	-
	
	
	

	
	
	
	
	


* Conversion factor for delivered electricity to primary energy = 2.4

	Operator’s comments :









Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)


Permit Number:  EPR/UP3237CP			Operator: 		Solway Foods Limited

Facility: 	RF Brookes 				Form Number: 	Performance1 / 25/03/2022

Reporting of other performance indicators for the period DD/MM/YYYY to DD/MM/YYYY

	Parameter
	
	Units 
	

	
	
	
	

	Food/drink/milk products



	tonnes
	

	Hazardous waste 




	tonnes/tonne
	

	Non hazardous waste
	tonnes/tonne
	

	Effluent discharged to sewer
	m3/tonne
	







	Operator’s comments :








Signed …………………………………………………………….  		Date………………………..   	
	(Authorised to sign as representative of Operator)

